$ +----------------------------------------------------+
$ |          FICHERO GENERADO CON CTE-HE 2013          |
$ +----------------------------------------------------+
$
$ PROGRAM = LIDER
$
 "DATOS GENERALES" = GENERAL-DATA
     TYPE-HOUSING        = "Terciario"
     YEAR                = "B"
     TYPE-DEFINITION     = "Nuevo"
     COMUNITY            = "Castilla y León"
     CITY                = "Salamanca"
     TOWN                = "Villares de la Reina"
     ZONE                = "D2"
     ALTITUDE            =            813
     ArchivoMetSel       = "C:\Program Files\Programas CTE y CEE\Datos Climaticos\GENERICOS\zonaD2.bin"
     TIPOUSO             = "I_Alta-8h-Acondicionado"
     CLASEHIGROMETRIA    = "3"
     NUMRENHS3           = "1,00"
     NUM-VIVIENDAS       = 1
     VENTILACION-POR-DEFECTO = "SI"
     VALORES-VENTILACION = ( "1.00", "1.00", "1.00", "2.00" )
     VALORES-PORCENTAJES = ( 25.000000, 25.000000, 25.000000, 25.000000 )
     NAME-PROJECT        = "CEIP "
     USE-PROJECT         = "COLEGIO"
     POSTCODE-PROJECT    = "37184"
     WAY-PROJECT         = "C/"
     STREET-NAME-PROJECT = "ESCUELAS"
     NUMBER-PROJECT      = "15-58"
     BLOCK-PROJECT       = "- "
     STAIR-PROJECT       = "-"
     FLOOR-PROJECT       = "-"
     GATE-PROJECT        = "-"
     IMAGE-PROJECT       = "Especifique imagen para el edificio"
     TEST-PROJECT        = "(null)"
     CURRENT-STATE-PROJECT = "X"
     PROPOSED-AMENDMENT-PROJECT = " "
     CIF/NIF-AUTHOR      = "CIF/NIF"
     NAME-AUTHOR         = "Autor"
     DOMICILIO           = ""
     PROVINCE-AUTHOR     = "Provincia"
     POSTCODE-AUTHOR     = "Código Postal"
     PHONE-AUTHOR        = "-"
     LOCALITY-AUTHOR     = "Localidad"
     IMAGE-AUTHOR        = "Especifique imagen para el plano de situación del edificio"
     MESINIPERSOM        = "Junio"
     MESFINPERSOM        = "Septiembre"
     ..

$
$ ----------------------
$ Datos de Base de Datos
$ ----------------------
$
TEMPLARY = USER
$ ++++++++++++++++++++++++++++++
$           MATERIALES
$ ++++++++++++++++++++++++++++++
$ ++++++++++++++++++++++++++++++
$         CERRAMIENTOS
$ ++++++++++++++++++++++++++++++
"CUBIERTA" = LAYERS
    GROUP        = "CERRAMIENTOS COLEGIO VILLARES"
    NAME_CALENER = ""
    NAME-INTERNAL = "CUBIERTA"
    TYPE-DEFINITION = 1
    MATERIAL     = ("arena","PS","XPS_HFC_032","fieltro","betun_lamina","MORgt1450","MAL","asfal","FUc300")
    THICKNESS = ( 0.100000, 0.010000, 0.100000, 0.010000, 0.010000, 0.010000, 0.150000, 0.010000,            0.3)
    LIBRARY       =  NO
    UTIL          =  YES
    AISLAMIENTO  = YES    ESPESOR  = 0    IMAGE = ""
    DEFAULT = NO
    ESTANQUEIDAD = NO
    AISLANTE-COL = 1
    RELATION     =              0
    TRANSMITANCIA     =              0
    WEIGHT            =              0
    AISLANTE-POSITION = Exterior
..
"I_CUBIERTA" = LAYERS
    GROUP        = "CERRAMIENTOS COLEGIO VILLARES"
    NAME_CALENER = "I_"
    MATERIAL     = ("FUc300","asfal","MAL","MORgt1450","betun_lamina","fieltro","XPS_HFC_032","PS","arena")
    THICKNESS = ( 0.300000, 0.010000, 0.150000, 0.010000, 0.010000, 0.010000, 0.100000, 0.010000,            0.1)
    LIBRARY       =  NO
    UTIL          =  YES
..
"CERRAMIENTO TIPO" = LAYERS
    GROUP        = "CERRAMIENTOS COLEGIO VILLARES"
    NAME_CALENER = ""
    NAME-INTERNAL = "CERRAMIENTO TIPO"
    TYPE-DEFINITION = 1
    MATERIAL     = ("aluminio","clv_ver_2","LPmp_50","MORgt1450","MW_04","PYL","PYL")
    THICKNESS = ( 0.005000, 0.050000, 0.123000, 0.020000, 0.100000, 0.013000,          0.013)
    LIBRARY       =  NO
    UTIL          =  YES
    AISLAMIENTO  = YES    ESPESOR  = 0    IMAGE = ""
    DEFAULT = NO
    ESTANQUEIDAD = NO
    AISLANTE-COL = 1
    RELATION     =              0
    TRANSMITANCIA     =              0
    WEIGHT            =              0
    AISLANTE-POSITION = Exterior
..
"I_CERRAMIENTO TIPO" = LAYERS
    GROUP        = "CERRAMIENTOS COLEGIO VILLARES"
    NAME_CALENER = "I_"
    MATERIAL     = ("PYL","PYL","MW_04","MORgt1450","LPmp_50","clv_ver_2","aluminio")
    THICKNESS = ( 0.013000, 0.013000, 0.100000, 0.020000, 0.123000, 0.050000,          0.005)
    LIBRARY       =  NO
    UTIL          =  YES
..
"FORJADO SANITARIO" = LAYERS
    GROUP        = "CERRAMIENTOS COLEGIO VILLARES"
    NAME_CALENER = ""
    NAME-INTERNAL = "FORJADO SANITARIO"
    TYPE-DEFINITION = 1
    MATERIAL     = ("plaqGres","MORgt1450","XPS_CO2_042","XPS_CO2_042","FUc300")
    THICKNESS = ( 0.030000, 0.047000, 0.033000, 0.040000,            0.3)
    LIBRARY       =  NO
    UTIL          =  YES
    AISLAMIENTO  = YES    ESPESOR  = 0    IMAGE = ""
    DEFAULT = NO
    ESTANQUEIDAD = NO
    AISLANTE-COL = 1
    RELATION     =              0
    TRANSMITANCIA     =              0
    WEIGHT            =              0
    AISLANTE-POSITION = Exterior
..
"I_FORJADO SANITARIO" = LAYERS
    GROUP        = "CERRAMIENTOS COLEGIO VILLARES"
    NAME_CALENER = "I_"
    MATERIAL     = ("FUc300","XPS_CO2_042","XPS_CO2_042","MORgt1450","plaqGres")
    THICKNESS = ( 0.300000, 0.040000, 0.033000, 0.047000,           0.03)
    LIBRARY       =  NO
    UTIL          =  YES
..
"FORJADO INTERMEDIO" = LAYERS
    GROUP        = "CERRAMIENTOS COLEGIO VILLARES"
    NAME_CALENER = ""
    NAME-INTERNAL = "FORJADO INTERMEDIO"
    TYPE-DEFINITION = 1
    MATERIAL     = ("plaqGres","MORgt1450","XPS_CO2_042","XPS_CO2_042","FUc300","cnv_hor_10","tabFib350")
    THICKNESS = ( 0.030000, 0.047000, 0.033000, 0.040000, 0.300000, 0.050000,           0.02)
    LIBRARY       =  NO
    UTIL          =  YES
    AISLAMIENTO  = YES    ESPESOR  = 0    IMAGE = ""
    DEFAULT = NO
    ESTANQUEIDAD = NO
    AISLANTE-COL = 1
    RELATION     =              0
    TRANSMITANCIA     =              0
    WEIGHT            =              0
    AISLANTE-POSITION = Exterior
..
"I_FORJADO INTERMEDIO" = LAYERS
    GROUP        = "CERRAMIENTOS COLEGIO VILLARES"
    NAME_CALENER = "I_"
    MATERIAL     = ("tabFib350","cnv_hor_10","FUc300","XPS_CO2_042","XPS_CO2_042","MORgt1450","plaqGres")
    THICKNESS = ( 0.020000, 0.050000, 0.300000, 0.040000, 0.033000, 0.047000,           0.03)
    LIBRARY       =  NO
    UTIL          =  YES
..
"TABIQUERIA TIPO" = LAYERS
    GROUP        = "CERRAMIENTOS COLEGIO VILLARES"
    NAME_CALENER = ""
    NAME-INTERNAL = "TABIQUERIA TIPO"
    TYPE-DEFINITION = 1
    MATERIAL     = ("PYL","PYL","MW_04","PYL","MW_04","PYL","tabPart270")
    THICKNESS = ( 0.013000, 0.013000, 0.048000, 0.013000, 0.048000, 0.013000,          0.015)
    LIBRARY       =  NO
    UTIL          =  YES
    AISLAMIENTO  = YES    ESPESOR  = 0    IMAGE = ""
    DEFAULT = NO
    ESTANQUEIDAD = NO
    AISLANTE-COL = 1
    RELATION     =              0
    TRANSMITANCIA     =              0
    WEIGHT            =              0
    AISLANTE-POSITION = Exterior
..
"I_TABIQUERIA TIPO" = LAYERS
    GROUP        = "CERRAMIENTOS COLEGIO VILLARES"
    NAME_CALENER = "I_"
    MATERIAL     = ("tabPart270","PYL","MW_04","PYL","MW_04","PYL","PYL")
    THICKNESS = ( 0.015000, 0.013000, 0.048000, 0.013000, 0.048000, 0.013000,          0.013)
    LIBRARY       =  NO
    UTIL          =  YES
..
$ ++++++++++++++++++++++++++++++
$  ACRISTALAMIENTOS - VIDRIOS
$ ++++++++++++++++++++++++++++++
"SGG Climaplus Planitherm 6_16_5" = GLASS-TYPE
     GROUP             = "VILLARES"
     TYPE              = SHADING-COEF
     SHADING-COEF      =      0.8235294
     GLASS-CONDUCTANCE =            1.3
     NAME_CALENER      = ""
     LIBRARY       =  NO
    UTIL          =  YES
    ..
"VIDRIO COLADO TRASL" = GLASS-TYPE
     GROUP             = "VILLARES"
     TYPE              = SHADING-COEF
     SHADING-COEF      =      0.8235294
     GLASS-CONDUCTANCE =            1.7
     NAME_CALENER      = ""
     LIBRARY       =  NO
    UTIL          =  YES
    ..
$ ++++++++++++++++++++++++++++++
$            MARCOS
$ ++++++++++++++++++++++++++++++
 "COR 70 INDUSTRIAL" = NAME-FRAME
      GROUP         = "VILLARES"
      FRAME-WIDTH   =            0.1
      FRAME-CONDUCT =            2.5
      FRAME-ABS     =            0.7
      NAME_CALENER  = ""
                LIBRARY       = NO
    UTIL          =  YES
..
$ ++++++++++++++++++++++++++++++
$             HUECOS
$ ++++++++++++++++++++++++++++++
"VENTANAS" = GAP
     NAME           = "VENTANAS"
     TYPE           = 1
     GROUP          = "HUECOS COLEGIO VILLARES"
     GROUP-GLASS         = "VILLARES"
     GLASS-TYPE          = "SGG Climaplus Planitherm 6_16_5"
     GROUP-FRAME       = "VILLARES"
     NAME-FRAME        = "COR 70 INDUSTRIAL"
     PORCENTAGE        = 10.000000
     INF-COEF          = 27.000000
     NAME_CALENER      = ""
    VIGENCIA = ( "A", "B", "C", "D", "E", "F")
    IMAGE = ""
     TRANSMITANCIA       =            5.7
     SHADING-COEF        =           0.86
     SHADE-COEF-SUMMER   =              1
     SHADE-COEF-WINTER   =              1
     MARKER-SUMMER       =              1
     MARKER-WINTER       =              1
     LIBRARY           =  NO
     UTIL              =  YES
     ISDOOR            = NO
     DEFAULT           = NO
    ..
"PUERTAS" = GAP
     NAME           = "PUERTAS"
     TYPE           = 1
     GROUP          = "HUECOS COLEGIO VILLARES"
     GROUP-GLASS         = "VILLARES"
     GLASS-TYPE          = "SGG Climaplus Planitherm 6_16_5"
     GROUP-FRAME       = "VILLARES"
     NAME-FRAME        = "COR 70 INDUSTRIAL"
     PORCENTAGE        = 10.000000
     INF-COEF          = 27.000000
     NAME_CALENER      = ""
    VIGENCIA = ( "A", "B", "C", "D", "E", "F")
    IMAGE = ""
     TRANSMITANCIA       =            5.7
     SHADING-COEF        =           0.86
     SHADE-COEF-SUMMER   =              1
     SHADE-COEF-WINTER   =              1
     MARKER-SUMMER       =              1
     MARKER-WINTER       =              1
     LIBRARY           =  NO
     UTIL              =  YES
     ISDOOR            = YES
     DEFAULT           = NO
    ..
"UGLASS" = GAP
     NAME           = "UGLASS"
     TYPE           = 1
     GROUP          = "HUECOS COLEGIO VILLARES"
     GROUP-GLASS         = "VILLARES"
     GLASS-TYPE          = "VIDRIO COLADO TRASL"
     GROUP-FRAME       = "VILLARES"
     NAME-FRAME        = "COR 70 INDUSTRIAL"
     PORCENTAGE        = 10.000000
     INF-COEF          = 27.000000
     NAME_CALENER      = ""
    VIGENCIA = ( "A", "B", "C", "D", "E", "F")
    IMAGE = ""
     TRANSMITANCIA       =            5.7
     SHADING-COEF        =           0.86
     SHADE-COEF-SUMMER   =              1
     SHADE-COEF-WINTER   =              1
     MARKER-SUMMER       =              1
     MARKER-WINTER       =              1
     LIBRARY           =  NO
     UTIL              =  YES
     ISDOOR            = NO
     DEFAULT           = NO
    ..
$ -------------------------
$ Final de la base de datos
$ -------------------------
$
$ +--------------------+
$ | Espacio de Trabajo |
$ +--------------------+
$
"Espacio de Trabajo" = WORK-SPACE
    WIDTH      =             50
    HIGHT      =             50
    Z          =              0
    BULB-TRA   = "Default.bulb"
    BULB-REF   = "Default.bulb"
    TRAN       =              0
    REFL       =            0.7
      ..

$
$ +------------------------+
$ | Datos de Base de Datos |
$ +------------------------+
$

$ ------------------
$ Sombras exteriores
$ ------------------
$
$ --------------------
$ Sombras Del Edificio
$ --------------------
$
$ -----------------
$ Lineas Auxiliares
$ -----------------
$
$ ------
$ Planos
$ ------
$

$ ---------
$ POLIGONOS
$ ---------
$
"P01_Poligono1" = POLYGON
    V1   =( 41.91694, -6.977726 )
    V2   =( 41.91694, 8.726489 )
    V3   =( -0.2907453, 8.724521 )
    V4   =( -0.2907453, 22.43074 )
    V5   =( -13.29166, 22.43144 )
    V6   =( -13.29104, 15.21558 )
    V7   =( -16.03067, 15.21558 )
    V8   =( -16.03248, -4.977502 )
    V9   =( -12.43996, -4.977502 )
    V10  =( -12.44082, -11.0806 )
    V11  =( -13.29286, -11.08065 )
    V12  =( -13.29573, -28.98628 )
    V13  =( -16.03536, -28.98628 )
    V14  =( -16.03605, -40.53528 )
    V15  =( 13.24693, -40.53528 )
    V16  =( 13.24693, -30.96679 )
    V17  =( -0.2961229, -30.96679 )
    V18  =( -0.2980551, -11.08053 )
    V19  =( -1.667868, -11.08053 )
    V20  =( -1.667868, -6.968667 )
    ..
"P01_E01_Poligono1" = POLYGON
    V1   =( -13.29166, 17.22754 )
    V2   =( -11.26549, 17.22754 )
    V3   =( -11.26549, 22.43074 )
    V4   =( -13.29166, 22.43144 )
    ..
"P01_E02_Poligono2" = POLYGON
    V1   =( -8.388326, 17.22754 )
    V2   =( -8.388326, 22.43074 )
    V3   =( -11.26549, 22.43074 )
    V4   =( -11.26549, 17.22754 )
    ..
"P01_E03_Poligono3" = POLYGON
    V1   =( -6.713559, 17.22754 )
    V2   =( -6.713559, 22.43074 )
    V3   =( -8.388326, 22.43074 )
    V4   =( -8.388326, 17.22754 )
    ..
"P01_E04_Poligono4" = POLYGON
    V1   =( -5.038792, 17.22754 )
    V2   =( -5.038792, 22.43074 )
    V3   =( -6.713559, 22.43074 )
    V4   =( -6.713559, 17.22754 )
    ..
"P01_E05_Poligono5" = POLYGON
    V1   =( -0.2907453, 17.22754 )
    V2   =( -0.2907453, 22.43074 )
    V3   =( -5.038792, 22.43074 )
    V4   =( -5.038792, 17.22754 )
    ..
"P01_E06_Poligono1" = POLYGON
    V1   =( -6.126526, 9.048145 )
    V2   =( -6.126706, 15.53541 )
    V3   =( -0.2907453, 15.53538 )
    V4   =( -0.2907453, 17.22754 )
    V5   =( -13.29166, 17.22754 )
    V6   =( -13.29166, 15.53538 )
    V7   =( -10.14167, 15.56256 )
    V8   =( -7.944051, 15.53538 )
    V9   =( -7.890037, 9.156529 )
    ..
"P01_E07_Poligono2" = POLYGON
    V1   =( -16.03067, 15.21558 )
    V2   =( -16.03106, 10.81246 )
    V3   =( -10.05998, 10.81246 )
    V4   =( -10.14167, 15.56256 )
    V5   =( -13.29166, 15.53538 )
    V6   =( -13.29104, 15.21558 )
    ..
"P01_E08_Poligono3" = POLYGON
    V1   =( -10.05998, 10.81246 )
    V2   =( -7.916775, 10.83968 )
    V3   =( -7.944051, 15.53538 )
    V4   =( -10.14167, 15.56256 )
    ..
"P01_E09_Poligono1" = POLYGON
    V1   =( -6.126526, 9.048145 )
    V2   =( -0.2907453, 9.05792 )
    V3   =( -0.2907453, 15.53538 )
    V4   =( -6.126706, 15.53541 )
    ..
"P01_E10_Poligono2" = POLYGON
    V1   =( -16.03106, 10.81246 )
    V2   =( -16.03248, -4.977502 )
    V3   =( -12.43996, -4.977502 )
    V4   =( -7.808126, -5.300864 )
    V5   =( -7.890037, 9.156529 )
    V6   =( -7.916775, 10.83968 )
    V7   =( -10.05998, 10.81246 )
    ..
"P01_E11_Poligono1" = POLYGON
    V1   =( -3.211125, 2.068947 )
    V2   =( 1.900021, 2.06893 )
    V3   =( 1.900021, 8.726489 )
    V4   =( -0.2907453, 8.724521 )
    V5   =( -0.2907453, 9.05792 )
    V6   =( -3.211125, 9.096324 )
    ..
"P01_E12_Poligono2" = POLYGON
    V1   =( 1.900021, 2.06893 )
    V2   =( 21.5851, 2.068947 )
    V3   =( 21.58361, 8.726489 )
    V4   =( 1.900021, 8.726489 )
    ..
"P01_E13_Poligono3" = POLYGON
    V1   =( 0.04188859, -0.0004191025 )
    V2   =( -2.254887, 0.0564109 )
    V3   =( -2.221332, -4.364026 )
    V4   =( -0.0786238, -4.298584 )
    ..
"P01_E14_Poligono4" = POLYGON
    V1   =( -2.221332, -4.364026 )
    V2   =( -2.292151, -6.837599 )
    V3   =( -1.667868, -6.968667 )
    V4   =( 0.001760951, -6.968667 )
    V5   =( -0.0786238, -4.298584 )
    ..
"P01_E15_Poligono5" = POLYGON
    V1   =( 0.04188859, -0.0004191025 )
    V2   =( -0.0786238, -4.298584 )
    V3   =( 0.001760951, -6.968667 )
    V4   =( 3.017527, -6.968667 )
    V5   =( 3.003027, 0.04234926 )
    ..
"P01_E16_Poligono6" = POLYGON
    V1   =( 3.003027, 0.04234926 )
    V2   =( 3.017527, -6.968667 )
    V3   =( 5.962257, -6.968667 )
    V4   =( 5.919407, -0.000782019 )
    ..
"P01_E17_Poligono7" = POLYGON
    V1   =( 5.919407, -0.000782019 )
    V2   =( 5.962257, -6.968667 )
    V3   =( 13.68067, -6.968667 )
    V4   =( 13.68088, 0.128164 )
    ..
"P01_E18_Poligono8" = POLYGON
    V1   =( 13.68088, 0.128164 )
    V2   =( 13.68067, -6.968667 )
    V3   =( 21.48483, -6.968667 )
    V4   =( 21.44269, 0.08525665 )
    ..
"P01_E19_Poligono1" = POLYGON
    V1   =( 24.7054, 8.726489 )
    V2   =( 21.58361, 8.726489 )
    V3   =( 21.5851, 2.068947 )
    V4   =( 1.900021, 2.06893 )
    V5   =( -3.211125, 2.068947 )
    V6   =( -3.211125, 9.096324 )
    V7   =( -6.126526, 9.048145 )
    V8   =( -7.890037, 9.156529 )
    V9   =( -7.808126, -5.300864 )
    V10  =( -12.43996, -4.977502 )
    V11  =( -12.44082, -11.0806 )
    V12  =( -7.801568, -10.75668 )
    V13  =( -5.79701, -10.75591 )
    V14  =( -1.667868, -11.08053 )
    V15  =( -1.667868, -6.968667 )
    V16  =( -2.292151, -6.837599 )
    V17  =( -2.221332, -4.364026 )
    V18  =( -2.254887, 0.0564109 )
    V19  =( 0.04188859, -0.0004191025 )
    V20  =( 3.003027, 0.04234926 )
    V21  =( 5.919407, -0.000782019 )
    V22  =( 13.68088, 0.128164 )
    V23  =( 21.44269, 0.08525665 )
    V24  =( 21.48483, -6.968667 )
    V25  =( 24.7054, -6.968667 )
    ..
"P01_E20_Poligono1" = POLYGON
    V1   =( -13.29286, -11.08065 )
    V2   =( -13.29436, -20.42631 )
    V3   =( -7.796886, -20.42631 )
    V4   =( -7.801568, -10.75668 )
    V5   =( -12.44082, -11.0806 )
    ..
"P01_E21_Poligono2" = POLYGON
    V1   =( -13.29436, -20.42631 )
    V2   =( -13.29484, -23.41586 )
    V3   =( -7.796886, -23.41586 )
    V4   =( -7.796886, -20.42631 )
    ..
"P01_E22_Poligono3" = POLYGON
    V1   =( -13.29484, -23.41586 )
    V2   =( -13.29531, -26.37256 )
    V3   =( -7.796886, -26.37256 )
    V4   =( -7.796886, -23.41586 )
    ..
"P01_E23_Poligono4" = POLYGON
    V1   =( -13.29531, -26.37256 )
    V2   =( -13.29573, -28.98628 )
    V3   =( -13.60843, -30.18341 )
    V4   =( -7.796886, -30.18341 )
    V5   =( -7.796886, -26.37256 )
    ..
"P01_E24_Poligono5" = POLYGON
    V1   =( -5.79701, -10.75591 )
    V2   =( -5.794036, -14.84144 )
    V3   =( -0.2976897, -14.84143 )
    V4   =( -0.2980551, -11.08053 )
    V5   =( -1.667868, -11.08053 )
    ..
"P01_E25_Poligono6" = POLYGON
    V1   =( -5.794036, -14.84144 )
    V2   =( -5.794036, -16.87827 )
    V3   =( -0.2974918, -16.87827 )
    V4   =( -0.2976897, -14.84143 )
    ..
"P01_E26_Poligono7" = POLYGON
    V1   =( -5.794036, -16.87827 )
    V2   =( -5.794036, -22.62741 )
    V3   =( -0.2969332, -22.62741 )
    V4   =( -0.2974918, -16.87827 )
    ..
"P01_E27_Poligono8" = POLYGON
    V1   =( -5.794036, -22.62741 )
    V2   =( -5.794036, -24.66424 )
    V3   =( -0.2967353, -24.66424 )
    V4   =( -0.2969332, -22.62741 )
    ..
"P01_E28_Poligono9" = POLYGON
    V1   =( -5.794036, -24.66424 )
    V2   =( -5.794036, -27.62094 )
    V3   =( -0.296448, -27.62094 )
    V4   =( -0.2967353, -24.66424 )
    ..
"P01_E29_Poligono10" = POLYGON
    V1   =( -5.794036, -27.62094 )
    V2   =( -5.794036, -29.26355 )
    V3   =( -0.2962884, -29.26355 )
    V4   =( -0.296448, -27.62094 )
    ..
"P01_E30_Poligono11" = POLYGON
    V1   =( -5.794036, -29.26355 )
    V2   =( -5.794036, -30.97187 )
    V3   =( -0.2961229, -30.96679 )
    V4   =( -0.2962884, -29.26355 )
    ..
"P01_E31_Poligono12" = POLYGON
    V1   =( -16.03536, -32.60329 )
    V2   =( -16.03605, -40.53528 )
    V3   =( -8.650287, -40.53528 )
    V4   =( -8.650287, -32.60329 )
    ..
"P01_E32_Poligono13" = POLYGON
    V1   =( -8.650287, -32.60329 )
    V2   =( -8.650287, -40.53528 )
    V3   =( -1.197059, -40.53528 )
    V4   =( -1.197059, -32.60329 )
    ..
"P01_E33_Poligono14" = POLYGON
    V1   =( -1.197059, -32.60329 )
    V2   =( -1.197059, -40.53528 )
    V3   =( 6.190501, -40.53528 )
    V4   =( 6.190501, -32.60329 )
    ..
"P01_E34_Poligono15" = POLYGON
    V1   =( 6.190501, -32.60329 )
    V2   =( 6.190501, -40.53528 )
    V3   =( 13.24693, -40.53528 )
    V4   =( 13.24693, -30.96679 )
    V5   =( 6.190501, -30.96679 )
    ..
"P01_E35_Poligono16" = POLYGON
    V1   =( -16.03536, -32.60329 )
    V2   =( -8.650287, -32.60329 )
    V3   =( -1.197059, -32.60329 )
    V4   =( 6.190501, -32.60329 )
    V5   =( 6.190501, -30.96679 )
    V6   =( -0.2961229, -30.96679 )
    V7   =( -5.794036, -30.97187 )
    V8   =( -5.794036, -29.26355 )
    V9   =( -5.794036, -27.62094 )
    V10  =( -5.794036, -24.66424 )
    V11  =( -5.794036, -22.62741 )
    V12  =( -5.794036, -16.87827 )
    V13  =( -5.794036, -14.84144 )
    V14  =( -5.79701, -10.75591 )
    V15  =( -7.801568, -10.75668 )
    V16  =( -7.796886, -20.42631 )
    V17  =( -7.796886, -23.41586 )
    V18  =( -7.796886, -26.37256 )
    V19  =( -7.796886, -30.18341 )
    V20  =( -13.60843, -30.18341 )
    V21  =( -13.29573, -28.98628 )
    V22  =( -16.03536, -28.98628 )
    ..
"P01_E36_Poligono17" = POLYGON
    V1   =( 24.7054, 8.726489 )
    V2   =( 24.66097, 4.783458 )
    V3   =( 29.48821, 4.684338 )
    V4   =( 29.48821, 8.726489 )
    ..
"P01_E37_Poligono18" = POLYGON
    V1   =( 29.48821, 8.726489 )
    V2   =( 29.48821, 4.684338 )
    V3   =( 34.24908, 4.684338 )
    V4   =( 34.24908, 8.726489 )
    ..
"P01_E38_Poligono19" = POLYGON
    V1   =( 34.24908, 8.726489 )
    V2   =( 34.24908, 4.684338 )
    V3   =( 36.5146, 4.684338 )
    V4   =( 36.5146, 8.726489 )
    ..
"P01_E39_Poligono20" = POLYGON
    V1   =( 36.5146, 8.726489 )
    V2   =( 36.5146, 4.684338 )
    V3   =( 41.91694, 4.684338 )
    V4   =( 41.91694, 8.726489 )
    ..
"P01_E40_Poligono21" = POLYGON
    V1   =( 24.66097, 4.783458 )
    V2   =( 24.7054, -6.968667 )
    V3   =( 41.91694, -6.977726 )
    V4   =( 41.91694, 4.684338 )
    V5   =( 36.5146, 4.684338 )
    V6   =( 34.24908, 4.684338 )
    V7   =( 29.48821, 4.684338 )
    ..
"P02_Poligono1" = POLYGON
    V1   =( 41.91694, -6.977726 )
    V2   =( 41.91694, 4.932601 )
    V3   =( 24.66097, 4.783458 )
    V4   =( 24.7054, 8.726489 )
    V5   =( -0.2907453, 8.724521 )
    V6   =( -16.03124, 8.812572 )
    V7   =( -16.02662, -6.95381 )
    ..
"P02_E01_Poligono2" = POLYGON
    V1   =( -16.03124, 8.812572 )
    V2   =( -16.02926, 2.037954 )
    V3   =( -6.301317, 2.037955 )
    V4   =( -6.301621, 8.758145 )
    ..
"P02_E02_Poligono1" = POLYGON
    V1   =( -0.2907453, 8.724521 )
    V2   =( -3.210449, 8.740854 )
    V3   =( -3.211125, 2.068947 )
    V4   =( 1.900021, 2.06893 )
    V5   =( 1.900021, 8.726489 )
    ..
"P02_E03_Poligono2" = POLYGON
    V1   =( 1.900021, 8.726489 )
    V2   =( 1.900021, 2.06893 )
    V3   =( 5.569138, 2.06893 )
    V4   =( 5.523046, 8.726489 )
    ..
"P02_E04_Poligono3" = POLYGON
    V1   =( 5.523046, 8.726489 )
    V2   =( 5.569138, 2.06893 )
    V3   =( 13.56683, 2.06893 )
    V4   =( 13.56684, 8.726489 )
    ..
"P02_E05_Poligono4" = POLYGON
    V1   =( 13.56684, 8.726489 )
    V2   =( 13.56683, 2.06893 )
    V3   =( 21.5851, 2.068947 )
    V4   =( 21.58361, 8.726489 )
    ..
"P02_E06_Poligono1" = POLYGON
    V1   =( -16.02868, 0.07062379 )
    V2   =( -16.02662, -6.95381 )
    V3   =( -7.898411, -6.95381 )
    V4   =( -7.838561, 0.0709613 )
    ..
"P02_E07_Poligono2" = POLYGON
    V1   =( -6.79527, 0.07062221 )
    V2   =( -6.79527, -4.252455 )
    V3   =( -5.140563, -4.252455 )
    V4   =( -5.140563, 0.07062221 )
    ..
"P02_E08_Poligono3" = POLYGON
    V1   =( -7.838561, 0.0709613 )
    V2   =( -7.898411, -6.95381 )
    V3   =( -5.140563, -6.95381 )
    V4   =( -5.140563, -4.252455 )
    V5   =( -6.79527, -4.252455 )
    V6   =( -6.79527, 0.07062221 )
    ..
"P02_E09_Poligono4" = POLYGON
    V1   =( -5.140563, 0.07062221 )
    V2   =( -5.140563, -4.252455 )
    V3   =( -5.140563, -6.95381 )
    V4   =( -2.292151, -6.837599 )
    V5   =( -2.254887, 0.0564109 )
    ..
"P02_E10_Poligono5" = POLYGON
    V1   =( -2.254887, 0.0564109 )
    V2   =( -2.292151, -6.837599 )
    V3   =( 1.524234, -6.95381 )
    V4   =( 1.524369, 0.02099268 )
    ..
"P02_E11_Poligono6" = POLYGON
    V1   =( 1.524369, 0.02099268 )
    V2   =( 1.524234, -6.95381 )
    V3   =( 9.338137, -6.95381 )
    V4   =( 9.292431, 0.05525608 )
    ..
"P02_E12_Poligono7" = POLYGON
    V1   =( 9.292431, 0.05525608 )
    V2   =( 9.338137, -6.95381 )
    V3   =( 17.01415, -6.95381 )
    V4   =( 16.96791, 0.1099933 )
    ..
"P02_E13_Poligono8" = POLYGON
    V1   =( 16.96791, 0.1099933 )
    V2   =( 17.01415, -6.95381 )
    V3   =( 24.7054, -6.968667 )
    V4   =( 24.7054, 0.07062221 )
    ..
"P02_E15_Poligono10" = POLYGON
    V1   =( 24.7054, 8.726489 )
    V2   =( 21.58361, 8.726489 )
    V3   =( 21.5851, 2.068947 )
    V4   =( 13.56683, 2.06893 )
    V5   =( 5.569138, 2.06893 )
    V6   =( 1.900021, 2.06893 )
    V7   =( -3.211125, 2.068947 )
    V8   =( -3.210449, 8.740854 )
    V9   =( -6.301621, 8.758145 )
    V10  =( -6.301317, 2.037955 )
    V11  =( -16.02926, 2.037954 )
    V12  =( -16.02868, 0.07062379 )
    V13  =( -7.838561, 0.0709613 )
    V14  =( -6.79527, 0.07062221 )
    V15  =( -5.140563, 0.07062221 )
    V16  =( -2.254887, 0.0564109 )
    V17  =( 1.524369, 0.02099268 )
    V18  =( 9.292431, 0.05525608 )
    V19  =( 16.96791, 0.1099933 )
    V20  =( 24.7054, 0.07062221 )
    V21  =( 24.66097, 4.783458 )
    ..
"P02_E01_FI001_Poligono11" = POLYGON
    V1   =( 0, 0 )
    V2   =( 8.1434, 0.0454998 )
    V3   =( 8.1815, 6.7746 )
    V4   =( 0.002000809, 6.7746 )
    V5   =( 0, 0.05910015 )
    ..
"P02_E01_FI002_Poligono12" = POLYGON
    V1   =( 0, 0 )
    V2   =( 6.7291, -0.03810024 )
    V3   =( 6.7202, 1.5481 )
    V4   =( 0, 1.5484 )
    ..
"P02_E06_FI007_Poligono17" = POLYGON
    V1   =( 0, 0 )
    V2   =( 8.190101, 0.00197137 )
    V3   =( 8.1901, 0.004071368 )
    V4   =( 8.142812, 5.368358 )
    V5   =( 3.5873, 5.049095 )
    V6   =( 1.636226e-11, 5.0481 )
    ..
"P02_E06_FI008_Poligono18" = POLYGON
    V1   =( 0, 0 )
    V2   =( 1.9763, 0.0002994537 )
    V3   =( 1.6583, 4.5559 )
    V4   =( 0, 4.5418 )
    ..
"P02_E06_FE001_Poligono19" = POLYGON
    V1   =( 0, 0 )
    V2   =( 1.9763, 9.892989e-12 )
    V3   =( 1.976844, 3.5864 )
    V4   =( 0.0005435563, 3.5873 )
    ..
"P02_E08_FI010_Poligono21" = POLYGON
    V1   =( 0, 0 )
    V2   =( 0.07624248, 5.369145 )
    V3   =( -1.545775e-09, 5.364495 )
    ..
"P02_E08_FI011_Poligono22" = POLYGON
    V1   =( 0, 0 )
    V2   =( 1.0433, 0.0002999976 )
    V3   =( 1.0433, 4.3233 )
    V4   =( 2.698, 4.3233 )
    V5   =( 2.698, 7.0247 )
    V6   =( -0.05989981, 7.0247 )
    V7   =( -0.04580021, 5.3664 )
    V8   =( 0.0303998, 5.3717 )
    V9   =( 0, 0.002099998 )
    ..
"P02_E10_FI013_Poligono24" = POLYGON
    V1   =( 0, 0 )
    V2   =( 4.299763, 0.01409417 )
    V3   =( 4.41822, 2.15452 )
    V4   =( 4.215139e-10, 2.297302 )
    ..
"P02_E10_FI014_Poligono25" = POLYGON
    V1   =( 0, 0 )
    V2   =( 2.474509, -0.00452509 )
    V3   =( 2.605201, 2.135188 )
    V4   =( 2.509193e-11, 2.293063 )
    ..
"P02_E10_FI015_Poligono26" = POLYGON
    V1   =( 0, 0 )
    V2   =( 2.605193, -0.1580104 )
    V3   =( 6.904966, -0.168723 )
    V4   =( 6.971359, 1.30914 )
    V5   =( 6.97146, 1.312438 )
    V6   =( -1.065087e-09, 1.525009 )
    ..
"P02_E10_FI016_Poligono27" = POLYGON
    V1   =( 0, 0 )
    V2   =( 0.0574162, 4.420154 )
    V3   =( 1.308826e-09, 6.894001 )
    ..
"P02_E11_FI001_Poligono1" = POLYGON
    V1   =( 0, 0 )
    V2   =( 1.4787, -0.006521204 )
    V3   =( 1.4933, 6.974679 )
    V4   =( 2.70157e-12, 6.9747 )
    ..
"P02_E11_FI002_Poligono2" = POLYGON
    V1   =( 0, 0 )
    V2   =( 6.9812, -0.0144999 )
    V3   =( 6.9847, 0.7617002 )
    V4   =( 6.9531, 2.9019 )
    V5   =( 0, 2.9446 )
    ..
"P02_E11_FI003_Poligono3" = POLYGON
    V1   =( 0, 0 )
    V2   =( 6.9531, -0.04269981 )
    V3   =( 7.009, 3.3242 )
    V4   =( 7.009, 3.3303 )
    V5   =( 0, 3.376 )
    ..
"P02_E11_FI004_Poligono4" = POLYGON
    V1   =( 0, 0 )
    V2   =( 0.0410432, 3.367113 )
    V3   =( 8.929512e-10, 5.507154 )
    ..
"P02_E12_FI005_Poligono5" = POLYGON
    V1   =( 0, 0 )
    V2   =( 4.388511, -0.0026867 )
    V3   =( 4.342407, 7.037463 )
    V4   =( -9.444174e-10, 7.009149 )
    ..
"P02_E12_FI006_Poligono6" = POLYGON
    V1   =( 0, 0 )
    V2   =( 7.0403, 0.0002002716 )
    V3   =( 7.0637, 3.287299 )
    V4   =( 0, 3.333499 )
    ..
"P02_E13_FI007_Poligono7" = POLYGON
    V1   =( 0, 0 )
    V2   =( 0.07139745, 0.0008669795 )
    V3   =( 4.474443, 0.05396542 )
    V4   =( 4.470549, 7.101691 )
    V5   =( 4.817597e-10, 7.063851 )
    ..
"P02_E13_FI008_Poligono8" = POLYGON
    V1   =( 0, 0 )
    V2   =( 7.047505, -0.05576701 )
    V3   =( 7.063329, -4.459105 )
    V4   =( 7.039187, 3.207055 )
    V5   =( 1.548441e-10, 3.220606 )
    ..
"P02_E15_FI007_Poligono7" = POLYGON
    V1   =( 0, 0 )
    V2   =( 1.967, -0.01119995 )
    V3   =( 1.9673, 8.178901 )
    V4   =( 0, 8.1795 )
    ..
"P02_E15_FI001_Poligono1" = POLYGON
    V1   =( 0, 0 )
    V2   =( 3.943, 0.04450035 )
    V3   =( 8.655801, 0 )
    V4   =( 8.6169, 7.6661 )
    V5   =( 8.616501, 7.737501 )
    V6   =( 8.5983, 11.0246 )
    V7   =( 8.671201, 15.4191 )
    V8   =( 8.6955, 20.9262 )
    V9   =( 8.6841, 21.7024 )
    V10  =( 8.705501, 23.1844 )
    V11  =( 8.67, 26.9602 )
    V12  =( 8.655801, 29.8459 )
    V13  =( 8.655801, 31.5006 )
    V14  =( 8.6555, 32.5439 )
    V15  =( 6.6885, 32.5551 )
    V16  =( 6.6885, 31.0067 )
    V17  =( -0.03169918, 31.007 )
    V18  =( -0.01439953, 27.9165 )
    V19  =( 6.6575, 27.9165 )
    V20  =( 6.6575, 3.1203 )
    V21  =( 0, 3.121801 )
    ..
"P01_E10_FE010_Poligono10" = POLYGON
    V1   =( 0, 0 )
    V2   =( 1.9999, -1.411489e-12 )
    V3   =( 2.044584, 8.143405 )
    V4   =( 1.655085, 8.141167 )
    V5   =( -0.02801232, 8.114297 )
    V6   =( -0.0005979508, 5.9711 )
    ..
"P01_E11_FE001_Poligono1" = POLYGON
    V1   =( 0, 0 )
    V2   =( 0.3334007, 0 )
    V3   =( 0.3718004, 2.9204 )
    V4   =( 0.0163002, 2.9204 )
    V5   =( 0.0163002, 2.9197 )
    ..
"P01_E14_FE002_Poligono2" = POLYGON
    V1   =( 0, 0 )
    V2   =( 0.6379166, -2.789875e-10 )
    V3   =( 2.27178, 0.3431027 )
    V4   =( 2.257421, 0.4027242 )
    ..
"P01_E17_FE001_Poligono1" = POLYGON
    V1   =( 0, 0 )
    V2   =( 0.01479993, -7.227552e-13 )
    V3   =( 0.06702235, 7.718224 )
    V4   =( 0.05222309, 7.718324 )
    ..
"P01_E19_FE001_Poligono1" = POLYGON
    V1   =( 0, 0 )
    V2   =( 0.3555002, 0 )
    V3   =( 0.3073006, 2.9154 )
    V4   =( 0.4157, 4.6789 )
    V5   =( 0.02620029, 4.6767 )
    V6   =( 0.01729965, 3.0905 )
    ..
"P01_E19_FE002_Poligono1" = POLYGON
    V1   =( 0, -0 )
    V2   =( 7.2997, 0 )
    V3   =( 7.3003, 4.126699 )
    V4   =( 2.661, 3.8028 )
    V5   =( 0.6564999, 3.8021 )
    V6   =( -3.4727, 4.126699 )
    V7   =( -3.4727, 0.01479959 )
    V8   =( -2.8484, -0.1163001 )
    ..
"P01_E36_FE019_Poligono18" = POLYGON
    V1   =( 0, 0 )
    V2   =( 3.943252, -1.216687e-09 )
    V3   =( 3.847077, 4.826521 )
    V4   =( -0.0539748, 4.782494 )
    ..
"P01_E37_FE020_Poligono19" = POLYGON
    V1   =( 0, 0 )
    V2   =( 3.9013, 0 )
    V3   =( 3.8601, 4.760801 )
    V4   =( 0, 4.760801 )
    ..
"P01_E38_FE021_Poligono20" = POLYGON
    V1   =( 0, 0 )
    V2   =( 3.8601, 0 )
    V3   =( 3.8405, 2.265598 )
    V4   =( 0, 2.265598 )
    ..
"P01_E39_FE022_Poligono21" = POLYGON
    V1   =( 0, 0 )
    V2   =( 3.8405, 0 )
    V3   =( 3.7938, 5.402302 )
    V4   =( 0, 5.402302 )
    ..
"P01_E40_MCP001_Poligono1" = POLYGON
    V1   =( 0, 0 )
    V2   =( 0.04450217, -1.300293e-12 )
    V3   =( 0.001933147, 4.71301 )
    ..
"P01_E40_MCP002_Poligono2" = POLYGON
    V1   =( 0, -0 )
    V2   =( 0.1408, 0 )
    V3   =( 0.04170179, 4.827299 )
    ..
"P01_E40_MCP003_Poligono3" = POLYGON
    V1   =( 0, -0 )
    V2   =( 0.1820002, 0 )
    V3   =( 0.1820002, 4.760801 )
    V4   =( 0.04120016, 4.760801 )
    ..
"P01_E40_MCP004_Poligono4" = POLYGON
    V1   =( 0, -0 )
    V2   =( 0.2016001, 0 )
    V3   =( 0.2016001, 2.265598 )
    V4   =( 0.01959991, 2.265598 )
    ..
"P01_E40_MCP005_Poligono5" = POLYGON
    V1   =( 0, 0 )
    V2   =( 5.402302, 1.250042e-14 )
    V3   =( 5.402302, 0.2016015 )
    V4   =( 2.191634e-08, 0.2483001 )
    ..
"P01_E40_MCP006_Poligono6" = POLYGON
    V1   =( 0, 0 )
    V2   =( 4.713046, 0 )
    V3   =( 4.713046, 3.7 )
    V4   =( 0, 3.7 )
    ..
"P01_E40_MCP007_Poligono7" = POLYGON
    V1   =( 0, 0 )
    V2   =( 17.21154, 0 )
    V3   =( 17.21154, 3.7 )
    V4   =( 0, 3.7 )
    ..
"P01_E40_MCP008_Poligono8" = POLYGON
    V1   =( 0, 0 )
    V2   =( 11.91033, 0 )
    V3   =( 11.91033, 3.7 )
    V4   =( 0, 3.7 )
    ..
"P01_E40_MCP009_Poligono9" = POLYGON
    V1   =( 0, 0 )
    V2   =( 17.25662, 0 )
    V3   =( 17.25662, 3.7 )
    V4   =( 0, 3.7 )
    ..
"P01_E40_MCP010_Poligono10" = POLYGON
    V1   =( 0, 0 )
    V2   =( 4.713045, 5.310663e-10 )
    V3   =( 11.75202, -0.06636778 )
    V4   =( 11.92335, 17.14432 )
    V5   =( 0.01353602, 17.25661 )
    ..
$
$ +-------------------+
$ | DATOS GEOMÉTRICOS |
$ +-------------------+
$
         "Run Period 1" = RUN-PERIOD-PD
           END-MONTH = 12
           END-DAY   = 31
           ..
    "Edificio" = BUILD-PARAMETERS
$          NOMBRE    = "Edificio"
           LATITUDE  = 0.000000
           ALTITUDE  = 0.000000
           ISPENINSULAR  = YES
           AZIMUTH   = 17.000000
$          LOCALIDAD = "Villares de la Reina"
$          ZONE      = "-- Todas --"
           CLASE-HIGROMETRIA  = 3
           ANGLE              = 0.000000
$          COND-OPER = "I_Alta-8h-Acondicionado"
$          TYPE-OPER = "Ninguno"
           HEATING-PERIOD = (  1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12)
           COOLING-PERIOD = (  1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12)
    AIR-CHANGES/HR        = ( 0.8 )
    PERCENTAGE-AIR-CHANGES  = ( 100 )
           INTERNAL-PARTITIONS = CUSTOM
           TYPE-CASE          = Nuevo
           TYPE-BUILD         = Terciario
           STOP-AFTER-MINIMUM-REQUIREMENTS = "NO"
           LONGITUD-DE-REFERENCIA = 15.000000
           ALTITUD = 818.000000
           ..
"P01" = FLOOR
      POLYGON       =  "P01_Poligono1"
      FLOOR-HEIGHT  =            3.7
      SPACE-HEIGHT  =            3.7
      SHAPE         =  POLYGON
      PREVIOUS      =  "Ninguna"
      ..
    "P01_E01" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E01_Poligono1"
            TYPE              = UNCONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Baja-8h-No_acondicionado"
            SPACE-CONDITIONS  = "I_Baja-8h-No_acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E01_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E01_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E01_FE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E01_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E06"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E01_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E02"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E01_FTER019" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        67.64709
                   PERIMETRO     =        23.40802
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E02" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E02_Poligono2"
            TYPE              = UNCONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Baja-8h-No_acondicionado"
            SPACE-CONDITIONS  = "I_Baja-8h-No_acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E02_PE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E02_FE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E02_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E03"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E02_Med005" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E06"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E02_FTER018" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        67.64709
                   PERIMETRO     =        23.40802
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E03" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E03_Poligono3"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E03_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E03_PE001_V" = WINDOW
                        X              =           0.43
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E03_FE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E03_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E04"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E03_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E06"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E03_FTER017" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        67.64709
                   PERIMETRO     =        23.40802
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E04" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E04_Poligono4"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E04_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E04_PE001_V" = WINDOW
                        X              =           0.36
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E04_FE004" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E04_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E05"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E04_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E06"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E04_FTER016" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        67.64709
                   PERIMETRO     =        23.40802
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E05" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E05_Poligono5"
            TYPE              = UNCONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Baja-8h-No_acondicionado"
            SPACE-CONDITIONS  = "I_Baja-8h-No_acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E05_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E05_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E05_FE005" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E05_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E06"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E05_FTER015" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        67.64709
                   PERIMETRO     =        23.40802
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E06" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E06_Poligono1"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E06_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E06_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.4
                        WIDTH          =            1.6
                        GAP            = "PUERTAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.04921085
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E06_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V5  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E06_PE002_V" = WINDOW
                        X              =           0.01
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.4
                        WIDTH          =           1.67
                        GAP            = "PUERTAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.05049108
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E06_FE006" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E06_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E09"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E06_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E09"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E06_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E07"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V6  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E06_Med005" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E08"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V7  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E06_Med006" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E08"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V8  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E06_Med007" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V9  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E06_FTER014" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E07" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E07_Poligono2"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E07_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E07_PE001_V" = WINDOW
                        X              =            0.9
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =           3.13
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.06057425
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E07_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V5  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E07_PE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V6  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E07_PE003_V" = WINDOW
                        X              =           0.01
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.4
                        WIDTH          =              1
                        GAP            = "PUERTAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03605897
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E07_FE007" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E07_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E10"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E07_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E08"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E07_FTER020" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E08" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E08_Poligono3"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E08_FE008" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E08_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E10"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E08_FTER021" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E09" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E09_Poligono1"
            TYPE              = UNCONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Baja-8h-No_acondicionado"
            SPACE-CONDITIONS  = "I_Baja-8h-No_acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E09_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E09_FE009" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E09_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E09_FTER013" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E10" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E10_Poligono2"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E10_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E10_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =          15.77
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.08561458
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E10_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E10_PE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V5  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E10_FE010" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =        -16.031
                  Y             =        10.8124
                  Z             =            3.7
                  AZIMUTH       =            270
                  LOCATION      = TOP  
                  POLYGON       = "P01_E10_FE010_Poligono10"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E10_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E10_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E10_FTER022" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E11" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E11_Poligono1"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E11_PE004" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E11_PE004_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           2.17
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.05197877
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E11_PE005" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E11_FE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =        -0.2907
                  Y             =         8.7245
                  Z             =            3.7
                  AZIMUTH       =             90
                  LOCATION      = TOP  
                  POLYGON       = "P01_E11_FE001_Poligono1"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E11_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E11_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E12"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E11_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V6  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E11_FTER012" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E12" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E12_Poligono2"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E12_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E12_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =          19.66
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.08733557
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E12_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E12_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E12_FTER007" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E13" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E13_Poligono3"
            TYPE              = UNCONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Baja-8h-No_acondicionado"
            SPACE-CONDITIONS  = "I_Baja-8h-No_acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E13_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E13_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E13_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E14"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E13_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E13_FTER023" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E14" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E14_Poligono4"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E14_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E14_PE001_V" = WINDOW
                        X              =            0.5
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =            0.2
                        OVERHANG-W     =              0
                        OVERHANG-D     =              3
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E14_FE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =        -2.2921
                  Y             =        -6.8375
                  Z             =            3.7
                  AZIMUTH       =       191.8595
                  LOCATION      = TOP  
                  POLYGON       = "P01_E14_FE002_Poligono2"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E14_Med005" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E14_Med006" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E14_Med007" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E14_FTER024" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E15" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E15_Poligono5"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E15_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E15_PE001_V" = WINDOW
                        X              =            1.2
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           1.44
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.04201513
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E15_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E16"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E15_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V5  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E15_FTER011" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E16" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E16_Poligono6"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E16_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E16_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           2.92
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.05899607
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E16_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E17"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E16_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E16_FTER010" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E17" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E17_Poligono7"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E17_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E17_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =            7.7
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07744753
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E17_FE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =         5.9621
                  Y             =        -6.9538
                  Z             =            3.7
                  AZIMUTH       =       269.6124
                  LOCATION      = TOP  
                  POLYGON       = "P01_E17_FE001_Poligono1"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E17_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E18"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E17_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E17_FTER009" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E18" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E18_Poligono8"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E18_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E18_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           7.78
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07759739
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E18_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E18_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E18_FTER008" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E19" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E19_Poligono1"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E19_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E19_PE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V10  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E19_PE003_V" = WINDOW
                        X              =            0.3
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.4
                        WIDTH          =            5.5
                        GAP            = "PUERTAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.08539025
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              3
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E19_PE004" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V14  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E19_PE004_V" = WINDOW
                        X              =           0.01
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.4
                        WIDTH          =           4.09
                        GAP            = "PUERTAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07747371
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =            1.5
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E19_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V6  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E19_PE005" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V24  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E19_PE005_V" = WINDOW
                        X              =           0.01
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.4
                        WIDTH          =            3.2
                        GAP            = "PUERTAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07033839
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              5
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E19_FE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =        -3.2111
                  Y             =         8.7408
                  Z             =            3.7
                  AZIMUTH       =             90
                  LOCATION      = TOP  
                  POLYGON       = "P01_E19_FE001_Poligono1"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E19_FE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =        -5.1405
                  Y             =        -6.9538
                  Z             =            3.7
                  AZIMUTH       =              0
                  LOCATION      = TOP  
                  POLYGON       = "P01_E19_FE002_Poligono1"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E19_Med009" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E20"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V11  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E19_Med010" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V12  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E19_Med011" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E24"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V13  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E19_Med022" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E40"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V25  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E19_FTER006" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E20" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E20_Poligono1"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E20_PE006" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E20_PE006_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =           9.33
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.08006874
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              2
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              5
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E20_PE007" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V5  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E20_FE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E20_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E21"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E20_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E20_FTER025" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E21" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E21_Poligono2"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E21_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E21_PE001_V" = WINDOW
                        X              =           1.07
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              2
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E21_FE004" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E21_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E22"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E21_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E21_FTER030" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E22" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E22_Poligono3"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E22_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E22_PE001_V" = WINDOW
                        X              =           0.72
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              2
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E22_FE005" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E22_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E23"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E22_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E22_FTER031" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E23" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E23_Poligono4"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E23_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E23_PE001_V" = WINDOW
                        X              =              1
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              2
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E23_FE006" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E23_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E23_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E23_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E23_FTER032" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E24" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E24_Poligono5"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E24_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E24_PE001_V" = WINDOW
                        X              =            2.6
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
                  "P01_E24_PE001_V_1" = WINDOW
                        X              =           0.64
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E24_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E24_FE007" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E24_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E24_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E25"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E24_FTER027" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E25" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E25_Poligono6"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E25_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E25_PE001_V" = WINDOW
                        X              =           0.61
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E25_FE008" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E25_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E25_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E26"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E25_FTER028" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E26" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E26_Poligono7"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E26_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E26_PE001_V" = WINDOW
                        X              =            4.5
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
                  "P01_E26_PE001_V_1" = WINDOW
                        X              =           2.65
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
                  "P01_E26_PE001_V_2" = WINDOW
                        X              =           0.87
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E26_FE009" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E26_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E26_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E27"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E26_FTER029" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E27" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E27_Poligono8"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E27_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E27_PE001_V" = WINDOW
                        X              =            0.5
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E27_FE010" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E27_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E27_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E28"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E27_FTER033" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E28" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E28_Poligono9"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E28_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E28_PE001_V" = WINDOW
                        X              =           0.27
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
                  "P01_E28_PE001_V_1" = WINDOW
                        X              =           1.73
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E28_FE011" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E28_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E28_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E29"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E28_FTER034" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E29" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E29_Poligono10"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E29_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E29_PE001_V" = WINDOW
                        X              =           0.32
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E29_FE012" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E29_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E29_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E30"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E29_FTER035" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E30" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E30_Poligono11"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E30_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E30_PE001_V" = WINDOW
                        X              =           0.34
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =              1
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03353417
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E30_FE013" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E30_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E30_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E30_FTER038" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E31" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E31_Poligono12"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E31_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E31_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E31_PE002_V" = WINDOW
                        X              =           0.01
                        Y              =              0
                        SETBACK        =              0
                        HEIGHT         =           2.75
                        WIDTH          =           7.37
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =      0.1022001
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E31_FE014" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E31_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E32"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E31_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E31_FTER036" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E32" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E32_Poligono13"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E32_PE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E32_PE003_V" = WINDOW
                        X              =           0.01
                        Y              =              0
                        SETBACK        =              0
                        HEIGHT         =           2.75
                        WIDTH          =           7.43
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =      0.1024168
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E32_FE015" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E32_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E33"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E32_Med005" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E32_FTER037" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E33" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E33_Poligono14"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E33_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E33_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =              0
                        SETBACK        =              0
                        HEIGHT         =           2.75
                        WIDTH          =           7.37
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =      0.1022001
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E33_FE016" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E33_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E34"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E33_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E33_FTER039" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E34" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E34_Poligono15"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E34_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E34_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =              0
                        SETBACK        =              0
                        HEIGHT         =           2.75
                        WIDTH          =           7.04
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =      0.1009587
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P01_E34_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E34_PE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E34_FE017" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E34_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E35"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V5  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E34_FTER040" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E35" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E35_Poligono16"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E35_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V5  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E35_PE001_V" = WINDOW
                        X              =            0.1
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =            5.2
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07099736
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
                  "P01_E35_PE001_V_1" = WINDOW
                        X              =            5.4
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.4
                        WIDTH          =              1
                        GAP            = "PUERTAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.03605897
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E35_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V21  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E35_PE002_V" = WINDOW
                        X              =            0.2
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.4
                        WIDTH          =            2.4
                        GAP            = "PUERTAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.06158004
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E35_PE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V22  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E35_PE003_V" = WINDOW
                        X              =              2
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.4
                        WIDTH          =            1.6
                        GAP            = "PUERTAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.04921085
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E35_FE018" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E35_FTER026" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        1348.987
                   PERIMETRO     =        205.3215
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E36" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E36_Poligono17"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E36_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E36_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =           2.25
                        SETBACK        =            0.3
                        HEIGHT         =            0.6
                        WIDTH          =           4.76
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.02691204
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E36_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E36_FE019" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =        24.7054
                  Y             =         8.7264
                  Z             =            3.7
                  AZIMUTH       =       270.6465
                  LOCATION      = TOP  
                  POLYGON       = "P01_E36_FE019_Poligono18"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E36_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E40"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E36_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E37"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E36_FTER005" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        270.5645
                   PERIMETRO     =        50.12738
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E37" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E37_Poligono18"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E37_PE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E37_PE003_V" = WINDOW
                        X              =           0.01
                        Y              =           2.25
                        SETBACK        =            0.3
                        HEIGHT         =            0.6
                        WIDTH          =           4.74
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.02690023
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E37_FE020" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =        29.4882
                  Y             =         8.7264
                  Z             =            3.7
                  AZIMUTH       =            270
                  LOCATION      = TOP  
                  POLYGON       = "P01_E37_FE020_Poligono19"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E37_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E40"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E37_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E38"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E37_FTER004" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        270.5645
                   PERIMETRO     =        50.12738
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E38" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E38_Poligono19"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E38_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E38_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =           2.25
                        SETBACK        =            0.3
                        HEIGHT         =            0.6
                        WIDTH          =           2.25
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.02409151
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E38_FE021" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =         34.249
                  Y             =         8.7264
                  Z             =            3.7
                  AZIMUTH       =            270
                  LOCATION      = TOP  
                  POLYGON       = "P01_E38_FE021_Poligono20"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E38_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E40"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E38_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E39"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E38_FTER003" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        270.5645
                   PERIMETRO     =        50.12738
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E39" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E39_Poligono20"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E39_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E39_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E39_PE002_V" = WINDOW
                        X              =            0.3
                        Y              =           2.25
                        SETBACK        =            0.3
                        HEIGHT         =            0.6
                        WIDTH          =              5
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.02704698
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E39_FE022" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =        36.5146
                  Y             =         8.7264
                  Z             =            3.7
                  AZIMUTH       =            270
                  LOCATION      = TOP  
                  POLYGON       = "P01_E39_FE022_Poligono21"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E39_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E40"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E39_FTER002" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        270.5645
                   PERIMETRO     =        50.12738
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
    "P01_E40" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P01_E40_Poligono21"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Media-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Media-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
            AREA        =       203.8966
            VOLUME        =        1498.05
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P01_E40_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E40_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E40_PE002_V" = WINDOW
                        X              =           0.23
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.7
                        WIDTH          =            2.5
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.06661036
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              5
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
                  "P01_E40_PE002_V_1" = WINDOW
                        X              =           3.01
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.7
                        WIDTH          =            2.5
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.06661036
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              5
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
                  "P01_E40_PE002_V_2" = WINDOW
                        X              =           5.96
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.7
                        WIDTH          =            2.5
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.06661036
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              5
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
                  "P01_E40_PE002_V_3" = WINDOW
                        X              =            8.7
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.7
                        WIDTH          =            2.5
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.06661036
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              5
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
                  "P01_E40_PE002_V_4" = WINDOW
                        X              =           11.3
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.7
                        WIDTH          =            2.5
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.06661036
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              5
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
                  "P01_E40_PE002_V_5" = WINDOW
                        X              =             14
                        Y              =              0
                        SETBACK        =            0.3
                        HEIGHT         =            2.7
                        WIDTH          =            2.5
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.06661036
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              5
                        OVERHANG-ANGLE =             90
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E40_MCP007" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  X             =        24.7054
                  Y             =      -6.968667
                  Z             =            3.7
                  AZIMUTH       =        180.028
                  TILT          =             90
                  POLYGON       = "P01_E40_MCP007_Poligono7"
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E40_MCP008" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  X             =       41.91694
                  Y             =      -6.977726
                  Z             =            3.7
                  AZIMUTH       =             90
                  TILT          =             90
                  POLYGON       = "P01_E40_MCP008_Poligono8"
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P01_E40_MCP009" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.3
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  X             =       41.91694
                  Y             =       4.932601
                  Z             =            3.7
                  AZIMUTH       =       359.5046
                  TILT          =             90
                  POLYGON       = "P01_E40_MCP009_Poligono9"
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P01_E40_MCP009_V1" = WINDOW
                        X              =            0.4
                        Y              =            0.1
                        SETBACK        =              0
                        HEIGHT         =              3
                        WIDTH          =             16
                        GAP            = "UGLASS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "VIDRIO COLADO TRASL"
                        FRAME-WIDTH   =      0.1280415
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P01_E40_MCP010" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  X             =       24.66097
                  Y             =       4.783458
                  Z             =            7.4
                  AZIMUTH       =       269.4597
                  TILT          =              0
                  POLYGON       = "P01_E40_MCP010_Poligono10"
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P01_E40_MCP001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "FORJADO INTERMEDIO"  
                  X             =        24.6609
                  Y             =         4.7834
                  Z             =            3.7
                  AZIMUTH       =       179.4825
                  TILT          =            180
                  POLYGON       = "P01_E40_MCP001_Poligono1"
                        ..
                  "FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "FORJADO INTERMEDIO" 
                        ..
            "P01_E40_MCP002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E36"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "FORJADO INTERMEDIO"  
                  X             =        29.4882
                  Y             =         4.8251
                  Z             =            3.7
                  AZIMUTH       =            270
                  TILT          =            180
                  POLYGON       = "P01_E40_MCP002_Poligono2"
                        ..
                  "FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "FORJADO INTERMEDIO" 
                        ..
            "P01_E40_MCP003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E37"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "FORJADO INTERMEDIO"  
                  X             =         34.249
                  Y             =         4.8663
                  Z             =            3.7
                  AZIMUTH       =            270
                  TILT          =            180
                  POLYGON       = "P01_E40_MCP003_Poligono3"
                        ..
                  "FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "FORJADO INTERMEDIO" 
                        ..
            "P01_E40_MCP004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E38"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "FORJADO INTERMEDIO"  
                  X             =        36.5146
                  Y             =         4.8859
                  Z             =            3.7
                  AZIMUTH       =            270
                  TILT          =            180
                  POLYGON       = "P01_E40_MCP004_Poligono4"
                        ..
                  "FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "FORJADO INTERMEDIO" 
                        ..
            "P01_E40_MCP005" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E39"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "FORJADO INTERMEDIO"  
                  X             =        41.9169
                  Y             =         4.6843
                  Z             =            3.7
                  AZIMUTH       =              0
                  TILT          =            180
                  POLYGON       = "P01_E40_MCP005_Poligono5"
                        ..
                  "FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "FORJADO INTERMEDIO" 
                        ..
            "P01_E40_MCP006" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  X             =       24.66097
                  Y             =       4.783458
                  Z             =            3.7
                  AZIMUTH       =       269.4598
                  TILT          =             90
                  POLYGON       = "P01_E40_MCP006_Poligono6"
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P01_E40_FTER001" = UNDERGROUND-WALL
                  Z-GROUND      =              0
   COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_FORJADO SANITARIO"  
                  LOCATION      = BOTTOM  
                   AREA          =        270.5645
                   PERIMETRO     =        50.12738
                        ..
                  "I_FORJADO SANITARIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO SANITARIO" 
                        ..
"P02" = FLOOR
      Z             =             3.7
      POLYGON       =  "P02_Poligono1"
      FLOOR-HEIGHT  =            3.7
      SPACE-HEIGHT  =            3.7
      SHAPE         =  POLYGON
      PREVIOUS      =  "P01"
      ..
    "P02_E01" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E01_Poligono2"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E01_PE023" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P02_E01_PE024" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E01_PE024_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           9.71
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.08057136
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E01_FE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E01_FI001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E10"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =       -16.0312
                  Y             =         8.8125
                  Z             =              0
                  AZIMUTH       =            180
                  TILT          =            180
                  POLYGON       = "P02_E01_FI001_Poligono11"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E01_FI002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        -7.8497
                  Y             =         2.0379
                  Z             =              0
                  AZIMUTH       =             90
                  TILT          =            180
                  POLYGON       = "P02_E01_FI002_Poligono12"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E01_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E01_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E02" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E02_Poligono1"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E02_PE025" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E02_PE025_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =            2.9
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.05883831
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E02_PE026" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V5  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E02_PE026_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           2.17
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.05197877
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E02_FE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E02_FI003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E11"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  LOCATION      = BOTTOM  
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E02_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E02_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E02_Med005" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E03"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E03" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E03_Poligono2"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E03_PE027" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E03_PE027_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =            3.6
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.06365527
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E03_FE004" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E03_FI004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E12"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  LOCATION      = BOTTOM  
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E03_Med007" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E03_Med008" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E04"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E04" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E04_Poligono3"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E04_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E04_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           8.02
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07803205
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E04_FE006" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E04_FI005" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E12"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  LOCATION      = BOTTOM  
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E04_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E04_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E05"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E05" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E05_Poligono4"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E05_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E05_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =              8
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07799666
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E05_FE005" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E05_FI006" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E12"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  LOCATION      = BOTTOM  
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E05_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E05_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E06" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E06_Poligono1"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E06_FE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "I_CUBIERTA"  
                  X             =       -12.4399
                  Y             =        -4.9775
                  Z             =              0
                  AZIMUTH       =            270
                  TILT          =            180
                  POLYGON       = "P02_E06_FE001_Poligono19"
                        ..
                  "I_CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_CUBIERTA" 
                        ..
            "P02_E06_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P02_E06_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E06_PE002_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           8.11
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07818953
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E06_FE007" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E06_FI007" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E10"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =       -16.0286
                  Y             =         0.0706
                  Z             =              0
                  AZIMUTH       =       179.9802
                  TILT          =            180
                  POLYGON       = "P02_E06_FI007_Poligono17"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E06_FI008" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =       -12.4402
                  Y             =        -6.9538
                  Z             =              0
                  AZIMUTH       =             90
                  TILT          =            180
                  POLYGON       = "P02_E06_FI008_Poligono18"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E06_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E08"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E06_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E07" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E07_Poligono2"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E07_FE009" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E07_FI009" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  LOCATION      = BOTTOM  
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E07_Med001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E08"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E07_Med002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E08"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E07_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E09"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E07_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E08" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E08_Poligono3"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E08_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E08_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           2.74
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.05752551
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E08_FE008" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E08_FI010" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E10"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        -7.8385
                  Y             =         0.0688
                  Z             =              0
                  AZIMUTH       =        180.489
                  TILT          =            180
                  POLYGON       = "P02_E08_FI010_Poligono21"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E08_FI011" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        -7.8385
                  Y             =         0.0709
                  Z             =              0
                  AZIMUTH       =            180
                  TILT          =            180
                  POLYGON       = "P02_E08_FI011_Poligono22"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E08_Med007" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E09"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E08_Med010" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V6  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E09" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E09_Poligono4"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E09_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E09_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           2.83
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.05827527
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E09_FE010" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E09_FI012" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  LOCATION      = BOTTOM  
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E09_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E10"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E09_Med005" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V5  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E10" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E10_Poligono5"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E10_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E10_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =            3.8
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =       0.064807
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E10_FE011" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E10_FI013" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E13"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =         0.0418
                  Y             =        -0.0004
                  Z             =              0
                  AZIMUTH       =       271.4167
                  TILT          =            180
                  POLYGON       = "P02_E10_FI013_Poligono24"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E10_FI014" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E14"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        -2.2921
                  Y             =        -6.8375
                  Z             =              0
                  AZIMUTH       =       91.74433
                  TILT          =            180
                  POLYGON       = "P02_E10_FI014_Poligono25"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E10_FI015" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        -0.0001
                  Y             =        -6.9073
                  Z             =              0
                  AZIMUTH       =       91.74732
                  TILT          =            180
                  POLYGON       = "P02_E10_FI015_Poligono26"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E10_FI016" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        -2.2548
                  Y             =         0.0564
                  Z             =              0
                  AZIMUTH       =       180.3103
                  TILT          =            180
                  POLYGON       = "P02_E10_FI016_Poligono27"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E10_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E11"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E10_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E11" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E11_Poligono6"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E11_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E11_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           7.79
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07761594
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E11_FE012" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E11_FI001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =         1.5243
                  Y             =         0.0209
                  Z             =              0
                  AZIMUTH       =            180
                  TILT          =            180
                  POLYGON       = "P02_E11_FI001_Poligono1"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E11_FI002" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E16"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =         3.0175
                  Y             =        -6.9538
                  Z             =              0
                  AZIMUTH       =             90
                  TILT          =            180
                  POLYGON       = "P02_E11_FI002_Poligono2"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E11_FI003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E17"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =         5.9621
                  Y             =        -6.9538
                  Z             =              0
                  AZIMUTH       =             90
                  TILT          =            180
                  POLYGON       = "P02_E11_FI003_Poligono3"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E11_FI004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =         9.2863
                  Y             =         0.0552
                  Z             =              0
                  AZIMUTH       =       269.7472
                  TILT          =            180
                  POLYGON       = "P02_E11_FI004_Poligono4"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E11_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E12"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E11_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E12" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E12_Poligono7"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E12_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E12_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           7.66
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07737163
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E12_FE013" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E12_FI005" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E17"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =         9.2924
                  Y             =         0.0552
                  Z             =              0
                  AZIMUTH       =       179.6262
                  TILT          =            180
                  POLYGON       = "P02_E12_FI005_Poligono5"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E12_FI006" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E18"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        13.6806
                  Y             =        -6.9538
                  Z             =              0
                  AZIMUTH       =             90
                  TILT          =            180
                  POLYGON       = "P02_E12_FI006_Poligono6"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E12_Med003" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E13"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V3  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
            "P02_E12_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E13" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E13_Poligono8"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E13_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V2  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E13_PE001_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =              0
                        HEIGHT         =            1.9
                        WIDTH          =           7.67
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.07739066
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        POSITION-LAMAS      = Horizontal
                        LAMAS-WIDTH         =           0.15
                        LAMAS-DISTANCE      =            0.1
                        LAMAS-ANGLE         =              2
                        LAMAS-TRANSMISIVITY =              0
                        LAMAS-REFLECTIVITY  =              0
                        ..
            "P02_E13_FE014" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E13_FI007" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E18"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        16.9679
                  Y             =         0.1099
                  Z             =              0
                  AZIMUTH       =       179.6252
                  TILT          =            180
                  POLYGON       = "P02_E13_FI007_Poligono7"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E13_FI008" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        21.4848
                  Y             =        -6.9624
                  Z             =              0
                  AZIMUTH       =        90.1103
                  TILT          =            180
                  POLYGON       = "P02_E13_FI008_Poligono8"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E13_Med004" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P02_E15"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "TABIQUERIA TIPO"  
                  LOCATION      = SPACE-V4  
                        ..
                  "TABIQUERIA TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "TABIQUERIA TIPO" 
                        ..
    "P02_E15" = SPACE
              HEIGHT        =            3.7
            SHAPE             = POLYGON 
            POLYGON           = "P02_E15_Poligono10"
            TYPE              = CONDITIONED
            SPACE-TYPE        = "Residencial"
            SYSTEM-CONDITIONS = "I_Alta-8h-Acondicionado"
            SPACE-CONDITIONS  = "I_Alta-8h-Acondicionado"
            FLOOR-WEIGHT      =              0
            MULTIPLIER        = 1
            MULTIPLIED        = 0
            PILLARS-NUMBERS   = 0
           INTERIOR-RADIATION  = FIXED
           CLASE-HIGROMETRIA  = 3
           POWER     = 4.400000
           VEEI-OBJ  = 7.000000
           VEEI-REF  = 10.000000
            ..
            "P02_E15_PE001" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V1  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E15_PE001_V" = WINDOW
                        X              =           0.92
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =            1.6
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.04456337
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P02_E15_PE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V8  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E15_PE002_V" = WINDOW
                        X              =            1.4
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =            1.9
                        WIDTH          =            1.6
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.04456337
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P02_E15_PE003" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.3
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V11  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
                  "P02_E15_PE003_V" = WINDOW
                        X              =           0.01
                        Y              =            0.9
                        SETBACK        =            0.3
                        HEIGHT         =           2.25
                        WIDTH          =           1.95
                        GAP            = "VENTANAS"
                        COEFF = ( 1.000000, 1.000000, 1.000000, 1.000000)
                        GLASS-TYPE     = "SGG Climaplus Planitherm 6_16_5"
                        FRAME-WIDTH   =     0.05360023
                        FRAME-CONDUCT =            2.5
                        FRAME-ABS     =            0.7
                        INF-COEF       =             27
                        OVERHANG-A     =              0
                        OVERHANG-B     =              0
                        OVERHANG-W     =              0
                        OVERHANG-D     =              0
                        OVERHANG-ANGLE =              0
                        LEFT-FIN-A     =              0
                        LEFT-FIN-B     =              0
                        LEFT-FIN-H     =              0
                        LEFT-FIN-D     =              0
                        RIGHT-FIN-A    =              0
                        RIGHT-FIN-B    =              0
                        RIGHT-FIN-H    =              0
                        RIGHT-FIN-D    =              0
                        ..
            "P02_E15_PE004" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CERRAMIENTO TIPO"  
                  LOCATION      = SPACE-V21  
                        ..
                  "CERRAMIENTO TIPO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CERRAMIENTO TIPO" 
                        ..
            "P02_E15_FE002" = EXTERIOR-WALL
                  ABSORPTANCE   =            0.6
                  COMPROBAR-REQUISITOS-MINIMOS = YES
                  CONSTRUCTION  = "CUBIERTA"  
                  LOCATION      = TOP  
                        ..
                  "CUBIERTA" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "CUBIERTA" 
                        ..
            "P02_E15_FI007" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E10"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        -7.8497
                  Y             =         2.0379
                  Z             =              0
                  AZIMUTH       =            270
                  TILT          =            180
                  POLYGON       = "P02_E15_FI007_Poligono7"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
            "P02_E15_FI001" = INTERIOR-WALL
                  INT-WALL-TYPE = STANDARD  
                  NEXT-TO       = "P01_E19"  
   COMPROBAR-REQUISITOS-MINIMOS = NO
                  CONSTRUCTION  = "I_FORJADO INTERMEDIO"  
                  X             =        24.7054
                  Y             =         8.7264
                  Z             =              0
                  AZIMUTH       =            270
                  TILT          =            180
                  POLYGON       = "P02_E15_FI001_Poligono1"
                        ..
                  "I_FORJADO INTERMEDIO" =  CONSTRUCTION
                        TYPE   = LAYERS  
                        LAYERS = "I_FORJADO INTERMEDIO" 
                        ..
$
$ +---------------------------+
$ | CONDICIONES OPERACIONALES |
$ +---------------------------+
$
"I_Baja-8h-No_acondicionado" = SPACE-CONDITIONS
    NAME               = "I_Baja-8h-No_acondicionado"
    TEMPERATURE        = 22.5
    PEOPLE-SCHEDULE    = "UsoEspacio-8h"
    PEOPLE-HG-LAT      =          45.42
    PEOPLE-HG-SENS     =             72
    PEOPLE-SPLIT-CR    =            0.4
    LIGHTING-SCHEDULE  = "UsoEspacio-8h"
    AREA/PERSON        =             36
    LIGHTING-TYPE      = SUS-FLUOR
    LIGHTING-W/AREA    =            1.5
    LIGHTING-SPLIT-CR =             0.5
    EQUIP-SCHEDULE        = "UsoEspacio-8h"
    EQUIP-SENSIBLE        =             90
    EQUIP-LATENT          =             10
    EQUIPMENT-SPLIT-CR    =            0.3
    EQUIPMENT-W/AREA      =            1.5
    FURN-FRACTION         =            0.5
    FURN-WEIGHT           =             30
    FRACCION-SOLAR-SUELO  =            0.6
    INF-SCHEDULE          = "UsoEspacio-8h_vent"
    INF-FLOW/AREA         =            7.2
    INF-METHOD            = CRACK-AIR-CHANGE
    PEAK-LOAD-TYPE        = CONDITIONED
    MET-LEVEL           = 1
      ..
"I_Baja-8h-No_acondicionado" = SYSTEM-CONDITIONS
    NAME               = "I_Baja-8h-No_acondicionado"
    ZONAL-ZONE-METHOD  = FULLY-MIXED
    HEAT-TEMP-SCH      = "Horario-Calefaccion-t"
    COOL-TEMP-SCH      = "Horario-Refrigeracion-t"
    TYPE               = UNCONDITIONED
    MAX-HEAT-RATE      = 0
    MAX-COOL-RATE      = 0
    HEATING-SCHEDULE   = "UsoEspacio-8h_eq"
    COOLING-SCHEDULE   = "UsoEspacio-8h_eq"
    FLOW/AREA          = 0
    FAN-SCHEDULE       = "UsoEspacio-8h_eq"
    SEASON-SCH         = "SSHA"
    OUTSIDE-AIR-FLOW   = 0
    RECOV-TEMP         = 0
    RECOV-KW           = 0
    RECOV-EFF          = 0
    THROTTLING-RANGE   = 0
    OA-CONTROL         = TEMP
            ..
"I_Media-8h-Acondicionado" = SPACE-CONDITIONS
    NAME               = "I_Media-8h-Acondicionado"
    TEMPERATURE        = 22.5
    PEOPLE-SCHEDULE    = "UsoEspacio-8h"
    PEOPLE-HG-LAT      =          45.42
    PEOPLE-HG-SENS     =             72
    PEOPLE-SPLIT-CR    =            0.4
    LIGHTING-SCHEDULE  = "UsoEspacio-8h"
    AREA/PERSON        =             12
    LIGHTING-TYPE      = SUS-FLUOR
    LIGHTING-W/AREA    =            4.5
    LIGHTING-SPLIT-CR =             0.5
    EQUIP-SCHEDULE        = "UsoEspacio-8h"
    EQUIP-SENSIBLE        =             90
    EQUIP-LATENT          =             10
    EQUIPMENT-SPLIT-CR    =            0.3
    EQUIPMENT-W/AREA      =            4.5
    FURN-FRACTION         =            0.5
    FURN-WEIGHT           =             30
    FRACCION-SOLAR-SUELO  =            0.6
    INF-SCHEDULE          = "UsoEspacio-8h_vent"
    INF-FLOW/AREA         =            7.2
    INF-METHOD            = CRACK-AIR-CHANGE
    PEAK-LOAD-TYPE        = CONDITIONED
    MET-LEVEL           = 1
      ..
"I_Media-8h-Acondicionado" = SYSTEM-CONDITIONS
    NAME               = "I_Media-8h-Acondicionado"
    ZONAL-ZONE-METHOD  = FULLY-MIXED
    HEAT-TEMP-SCH      = "Horario-Calefaccion-t"
    COOL-TEMP-SCH      = "Horario-Refrigeracion-t"
    TYPE               = CONDITIONED
    MAX-HEAT-RATE      = -1e20
    MAX-COOL-RATE      = 1e20
    HEATING-SCHEDULE   = "UsoEspacio-8h_eq"
    COOLING-SCHEDULE   = "UsoEspacio-8h_eq"
    FLOW/AREA          = 0
    FAN-SCHEDULE       = "UsoEspacio-8h_eq"
    SEASON-SCH         = "SSHA"
    OUTSIDE-AIR-FLOW   = 0
    RECOV-TEMP         = 0
    RECOV-KW           = 0
    RECOV-EFF          = 0
    THROTTLING-RANGE   = 0
    OA-CONTROL         = TEMP
            ..
"I_Alta-8h-Acondicionado" = SPACE-CONDITIONS
    NAME               = "I_Alta-8h-Acondicionado"
    TEMPERATURE        = 22.5
    PEOPLE-SCHEDULE    = "UsoEspacio-8h"
    PEOPLE-HG-LAT      =          45.42
    PEOPLE-HG-SENS     =             72
    PEOPLE-SPLIT-CR    =            0.4
    LIGHTING-SCHEDULE  = "UsoEspacio-8h"
    AREA/PERSON        =            7.2
    LIGHTING-TYPE      = SUS-FLUOR
    LIGHTING-W/AREA    =            7.5
    LIGHTING-SPLIT-CR =             0.5
    EQUIP-SCHEDULE        = "UsoEspacio-8h"
    EQUIP-SENSIBLE        =             90
    EQUIP-LATENT          =             10
    EQUIPMENT-SPLIT-CR    =            0.3
    EQUIPMENT-W/AREA      =            7.5
    FURN-FRACTION         =            0.5
    FURN-WEIGHT           =             30
    FRACCION-SOLAR-SUELO  =            0.6
    INF-SCHEDULE          = "UsoEspacio-8h_vent"
    INF-FLOW/AREA         =            7.2
    INF-METHOD            = CRACK-AIR-CHANGE
    PEAK-LOAD-TYPE        = CONDITIONED
    MET-LEVEL           = 1
      ..
"I_Alta-8h-Acondicionado" = SYSTEM-CONDITIONS
    NAME               = "I_Alta-8h-Acondicionado"
    ZONAL-ZONE-METHOD  = FULLY-MIXED
    HEAT-TEMP-SCH      = "Horario-Calefaccion-t"
    COOL-TEMP-SCH      = "Horario-Refrigeracion-t"
    TYPE               = CONDITIONED
    MAX-HEAT-RATE      = -1e20
    MAX-COOL-RATE      = 1e20
    HEATING-SCHEDULE   = "UsoEspacio-8h_eq"
    COOLING-SCHEDULE   = "UsoEspacio-8h_eq"
    FLOW/AREA          = 0
    FAN-SCHEDULE       = "UsoEspacio-8h_eq"
    SEASON-SCH         = "SSHA"
    OUTSIDE-AIR-FLOW   = 0
    RECOV-TEMP         = 0
    RECOV-KW           = 0
    RECOV-EFF          = 0
    THROTTLING-RANGE   = 0
    OA-CONTROL         = TEMP
            ..

"SSHDV" = DAY-SCHEDULE-PD
  TYPE  = FRACTION
  VALUES  = ( 0)
  ..
"SSHDI" = DAY-SCHEDULE-PD
  TYPE  = FRACTION
  VALUES  = ( 1)
  ..
"SSHSV" = WEEK-SCHEDULE-PD
  TYPE  = FRACTION
  DAY-SCHEDULES = ( "SSHDV")
  ..
"SSHSI" = WEEK-SCHEDULE-PD
  TYPE  = FRACTION
  DAY-SCHEDULES = ( "SSHDI")
  ..
"SSHA" = SCHEDULE-PD
  TYPE  = FRACTION
  MONTH = ( 5, 9, 12)
  DAY   = ( 31, 30, 31)
  WEEK-SCHEDULES = ( "SSHSI", "SSHSV", "SSHSI")
  ..
$
$ +----------+
$ | HORARIOS |
$ +----------+
$
"HA0_SS_D-Refrig-Temp-Lab" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 0
    VALUES  = ( 27.0, 27.0, 27.0, 27.0, 27.0, 27.0, 27.0, 99.0, 99.0, 99.0, 99.0, 99.0, 99.0, 99.0, 99.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 27.0)
    ..
"HA0_SS_D-Refrig-Temp-Sab" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 1
    VALUES  = ( 27.0, 27.0, 27.0, 27.0, 27.0, 27.0, 27.0, 99.0, 99.0, 99.0, 99.0, 99.0, 99.0, 99.0, 99.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 27.0)
    ..
"HA0_SS_D-Refrig-Temp-Fest" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 2
    VALUES  = ( 27.0, 27.0, 27.0, 27.0, 27.0, 27.0, 27.0, 99.0, 99.0, 99.0, 99.0, 99.0, 99.0, 99.0, 99.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 27.0)
    ..
  "HA0_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = TEMPERATURE
    DAY-SCHEDULES = ( "HA0_SS_D-Refrig-Temp-Lab",
                      "HA0_SS_D-Refrig-Temp-Lab",
                      "HA0_SS_D-Refrig-Temp-Lab",
                      "HA0_SS_D-Refrig-Temp-Lab",
                      "HA0_SS_D-Refrig-Temp-Lab",
                      "HA0_SS_D-Refrig-Temp-Sab",
                      "HA0_SS_D-Refrig-Temp-Fest")
    ..
"Horario-Refrigeracion" = SCHEDULE-PD
    TYPE   = "TEMPERATURE"
    GROUP  = "Temperaturas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA0_HS0_SS_")
    ..
"HA1_SS_D-Calef-Temp-Lab" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 0
    VALUES  = ( 17.0, 17.0, 17.0, 17.0, 17.0, 17.0, 17.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 17.0)
    ..
"HA1_SS_D-Calef-Temp-Sab" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 1
    VALUES  = ( 17.0, 17.0, 17.0, 17.0, 17.0, 17.0, 17.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 17.0)
    ..
"HA1_SS_D-Calef-Temp-Fest" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 2
    VALUES  = ( 17.0, 17.0, 17.0, 17.0, 17.0, 17.0, 17.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 17.0)
    ..
  "HA1_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = TEMPERATURE
    DAY-SCHEDULES = ( "HA1_SS_D-Calef-Temp-Lab",
                      "HA1_SS_D-Calef-Temp-Lab",
                      "HA1_SS_D-Calef-Temp-Lab",
                      "HA1_SS_D-Calef-Temp-Lab",
                      "HA1_SS_D-Calef-Temp-Lab",
                      "HA1_SS_D-Calef-Temp-Sab",
                      "HA1_SS_D-Calef-Temp-Fest")
    ..
"Horario-Calefaccion" = SCHEDULE-PD
    TYPE   = "TEMPERATURE"
    GROUP  = "Temperaturas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA1_HS0_SS_")
    ..
"HA2_SS_D-Refrig-Temp-Lab-t" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 0
    VALUES  = ( 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0)
    ..
"HA2_SS_D-Refrig-Temp-Sab-t" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 1
    VALUES  = ( 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0)
    ..
"HA2_SS_D-Refrig-Temp-Fest-t" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 2
    VALUES  = ( 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0, 25.0)
    ..
  "HA2_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = TEMPERATURE
    DAY-SCHEDULES = ( "HA2_SS_D-Refrig-Temp-Lab-t",
                      "HA2_SS_D-Refrig-Temp-Lab-t",
                      "HA2_SS_D-Refrig-Temp-Lab-t",
                      "HA2_SS_D-Refrig-Temp-Lab-t",
                      "HA2_SS_D-Refrig-Temp-Lab-t",
                      "HA2_SS_D-Refrig-Temp-Sab-t",
                      "HA2_SS_D-Refrig-Temp-Fest-t")
    ..
"Horario-Refrigeracion-t" = SCHEDULE-PD
    TYPE   = "TEMPERATURE"
    GROUP  = "Temperaturas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA2_HS0_SS_")
    ..
"HA3_SS_D-Calef-Temp-Lab-t" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 0
    VALUES  = ( 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0)
    ..
"HA3_SS_D-Calef-Temp-Sab-t" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 1
    VALUES  = ( 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0)
    ..
"HA3_SS_D-Calef-Temp-Fest-t" = DAY-SCHEDULE-PD
    TYPE  = "TEMPERATURE"
    GROUP = "Temperaturas"
    INDEX = 2
    VALUES  = ( 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0, 20.0)
    ..
  "HA3_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = TEMPERATURE
    DAY-SCHEDULES = ( "HA3_SS_D-Calef-Temp-Lab-t",
                      "HA3_SS_D-Calef-Temp-Lab-t",
                      "HA3_SS_D-Calef-Temp-Lab-t",
                      "HA3_SS_D-Calef-Temp-Lab-t",
                      "HA3_SS_D-Calef-Temp-Lab-t",
                      "HA3_SS_D-Calef-Temp-Sab-t",
                      "HA3_SS_D-Calef-Temp-Fest-t")
    ..
"Horario-Calefaccion-t" = SCHEDULE-PD
    TYPE   = "TEMPERATURE"
    GROUP  = "Temperaturas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA3_HS0_SS_")
    ..
"HA4_SS_D-8h-Lab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 0
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA4_SS_D-8h-Sab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 1
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA4_SS_D-8h-Fest" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 2
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
  "HA4_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA4_SS_D-8h-Lab",
                      "HA4_SS_D-8h-Lab",
                      "HA4_SS_D-8h-Lab",
                      "HA4_SS_D-8h-Lab",
                      "HA4_SS_D-8h-Lab",
                      "HA4_SS_D-8h-Sab",
                      "HA4_SS_D-8h-Fest")
    ..
"UsoEspacio-8h" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Internas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA4_HS0_SS_")
    ..
"HA5_SS_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 0
    VALUES  = ( 0, 0, 0, 0, 0, 0, 1, 1, 1, 1, 1, 1, 1, 1, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0)
    ..
"HA5_SS_D-8h-Sab_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 1
    VALUES  = ( 0, 0, 0, 0, 0, 0, 1, 1, 1, 1, 1, 1, 1, 1, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0)
    ..
"HA5_SS_D-8h-Fest_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 2
    VALUES  = ( 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0)
    ..
  "HA5_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = ON/OFF
    DAY-SCHEDULES = ( "HA5_SS_eq",
                      "HA5_SS_eq",
                      "HA5_SS_eq",
                      "HA5_SS_eq",
                      "HA5_SS_eq",
                      "HA5_SS_eq",
                      "HA5_SS_eq")
    ..
"UsoEspacio-8h_eq" = SCHEDULE-PD
    TYPE   = "ON/OFF"
    GROUP  = "Equipos"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA5_HS0_SS_")
    ..
"HA6_SS_vent" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 0
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA6_SS_D-8h-Sab_vent" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 1
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA6_SS_D-8h-Fest_vent" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 2
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
  "HA6_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA6_SS_vent",
                      "HA6_SS_vent",
                      "HA6_SS_vent",
                      "HA6_SS_vent",
                      "HA6_SS_vent",
                      "HA6_SS_vent",
                      "HA6_SS_vent")
    ..
"UsoEspacio-8h_vent" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Ventilación"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA6_HS0_SS_")
    ..
"HA7_SS_D-12h-Lab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 0
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA7_SS_D-12h-Sab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 1
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA7_SS_D-12h-Fest" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 2
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
  "HA7_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA7_SS_D-12h-Lab",
                      "HA7_SS_D-12h-Lab",
                      "HA7_SS_D-12h-Lab",
                      "HA7_SS_D-12h-Lab",
                      "HA7_SS_D-12h-Lab",
                      "HA7_SS_D-12h-Sab",
                      "HA7_SS_D-12h-Fest")
    ..
"UsoEspacio-12h" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Internas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA7_HS0_SS_")
    ..
"HA8_SS_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 0
    VALUES  = ( 0, 0, 0, 0, 0, 0, 1, 1, 1, 1, 1, 1, 1, 1, 0, 0, 1, 1, 1, 1, 0, 0, 0, 0)
    ..
"HA8_SS_D-12h-Sab_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 1
    VALUES  = ( 0, 0, 0, 0, 0, 0, 1, 1, 1, 1, 1, 1, 1, 1, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0)
    ..
"HA8_SS_D-12h-Fest_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 2
    VALUES  = ( 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0)
    ..
  "HA8_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = ON/OFF
    DAY-SCHEDULES = ( "HA8_SS_eq",
                      "HA8_SS_eq",
                      "HA8_SS_eq",
                      "HA8_SS_eq",
                      "HA8_SS_eq",
                      "HA8_SS_eq",
                      "HA8_SS_eq")
    ..
"UsoEspacio-12h_eq" = SCHEDULE-PD
    TYPE   = "ON/OFF"
    GROUP  = "Equipos"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA8_HS0_SS_")
    ..
"HA9_SS_D-12h-Lab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 0
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA9_SS_D-12h-Sab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 1
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA9_SS_D-12h-Fest" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 2
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
  "HA9_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA9_SS_D-12h-Lab",
                      "HA9_SS_D-12h-Lab",
                      "HA9_SS_D-12h-Lab",
                      "HA9_SS_D-12h-Lab",
                      "HA9_SS_D-12h-Lab",
                      "HA9_SS_D-12h-Sab",
                      "HA9_SS_D-12h-Fest")
    ..
"UsoEspacio-12h_vent" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Ventilación"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA9_HS0_SS_")
    ..
"HA10_SS_D-16h-Lab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 0
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00)
    ..
"HA10_SS_D-16h-Sab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 1
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA10_SS_D-16h-Fest" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 2
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
  "HA10_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA10_SS_D-16h-Lab",
                      "HA10_SS_D-16h-Lab",
                      "HA10_SS_D-16h-Lab",
                      "HA10_SS_D-16h-Lab",
                      "HA10_SS_D-16h-Lab",
                      "HA10_SS_D-16h-Sab",
                      "HA10_SS_D-16h-Fest")
    ..
"UsoEspacio-16h" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Internas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA10_HS0_SS_")
    ..
"HA11_SS_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 0
    VALUES  = ( 0, 0, 0, 0, 0, 0, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 0, 0)
    ..
"HA11_SS_D-16h-Sab_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 1
    VALUES  = ( 0, 0, 0, 0, 0, 0, 1, 1, 1, 1, 1, 1, 1, 1, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0)
    ..
"HA11_SS_D-16h-Fest_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 2
    VALUES  = ( 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0)
    ..
  "HA11_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = ON/OFF
    DAY-SCHEDULES = ( "HA11_SS_eq",
                      "HA11_SS_eq",
                      "HA11_SS_eq",
                      "HA11_SS_eq",
                      "HA11_SS_eq",
                      "HA11_SS_eq",
                      "HA11_SS_eq")
    ..
"UsoEspacio-16h_eq" = SCHEDULE-PD
    TYPE   = "ON/OFF"
    GROUP  = "Equipos"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA11_HS0_SS_")
    ..
"HA12_SS_vent" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 0
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00)
    ..
"HA12_SS_D-16h-Sab_vent" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 1
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA12_SS_D-16h-Fest_vent" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 2
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
  "HA12_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA12_SS_vent",
                      "HA12_SS_vent",
                      "HA12_SS_vent",
                      "HA12_SS_vent",
                      "HA12_SS_vent",
                      "HA12_SS_vent",
                      "HA12_SS_vent")
    ..
"UsoEspacio-16h_vent" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Ventilación"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA12_HS0_SS_")
    ..
"HA13_SS_D-24h-Lab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 0
    VALUES  = ( 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00)
    ..
"HA13_SS_D-24h-Sab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 1
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA13_SS_D-24h-Fest" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 2
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
  "HA13_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA13_SS_D-24h-Lab",
                      "HA13_SS_D-24h-Lab",
                      "HA13_SS_D-24h-Lab",
                      "HA13_SS_D-24h-Lab",
                      "HA13_SS_D-24h-Lab",
                      "HA13_SS_D-24h-Sab",
                      "HA13_SS_D-24h-Fest")
    ..
"UsoEspacio-24h" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Internas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA13_HS0_SS_")
    ..
"HA14_SS_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 0
    VALUES  = ( 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1)
    ..
"HA14_SS_D-24h-Sab_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 1
    VALUES  = ( 0, 0, 0, 0, 0, 0, 1, 1, 1, 1, 1, 1, 1, 1, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0)
    ..
"HA14_SS_D-24h-Fest_eq" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 2
    VALUES  = ( 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0)
    ..
  "HA14_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = ON/OFF
    DAY-SCHEDULES = ( "HA14_SS_eq",
                      "HA14_SS_eq",
                      "HA14_SS_eq",
                      "HA14_SS_eq",
                      "HA14_SS_eq",
                      "HA14_SS_eq",
                      "HA14_SS_eq")
    ..
"UsoEspacio-24h_eq" = SCHEDULE-PD
    TYPE   = "ON/OFF"
    GROUP  = "Equipos"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA14_HS0_SS_")
    ..
"HA15_SS_vent" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 0
    VALUES  = ( 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00)
    ..
"HA15_SS_D-24h-Sab_vent" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 1
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
"HA15_SS_D-24h-Fest_vent" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 2
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
  "HA15_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA15_SS_vent",
                      "HA15_SS_vent",
                      "HA15_SS_vent",
                      "HA15_SS_vent",
                      "HA15_SS_vent",
                      "HA15_SS_vent",
                      "HA15_SS_vent")
    ..
"UsoEspacio-24h_vent" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Ventilación"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA15_HS0_SS_")
    ..
"HA16_SS_D-Resid-Ocup-Lab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 0
    VALUES  = ( 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.50, 0.50, 0.50, 0.50, 0.50, 0.50, 0.50, 0.50, 1.00)
    ..
"HA16_SS_D-Resid-Ocup-Sab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 1
    VALUES  = ( 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00)
    ..
"HA16_SS_D-Resid-Ocup-Fest" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 2
    VALUES  = ( 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00)
    ..
  "HA16_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA16_SS_D-Resid-Ocup-Lab",
                      "HA16_SS_D-Resid-Ocup-Lab",
                      "HA16_SS_D-Resid-Ocup-Lab",
                      "HA16_SS_D-Resid-Ocup-Lab",
                      "HA16_SS_D-Resid-Ocup-Lab",
                      "HA16_SS_D-Resid-Ocup-Sab",
                      "HA16_SS_D-Resid-Ocup-Fest")
    ..
"Ocupacion-Residencia" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Internas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA16_HS0_SS_")
    ..
"HA17_SS_D-Resid-ilum-Lab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 0
    VALUES  = ( 0.10, 0.10, 0.10, 0.10, 0.10, 0.10, 0.10, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.50, 1.00, 1.00, 1.00, 1.00, 0.50)
    ..
"HA17_SS_D-Resid-ilum-Sab" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 1
    VALUES  = ( 0.10, 0.10, 0.10, 0.10, 0.10, 0.10, 0.10, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.50, 1.00, 1.00, 1.00, 1.00, 0.50)
    ..
"HA17_SS_D-Resid-ilum-Fest" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 2
    VALUES  = ( 0.10, 0.10, 0.10, 0.10, 0.10, 0.10, 0.10, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.30, 0.50, 1.00, 1.00, 1.00, 1.00, 0.50)
    ..
  "HA17_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA17_SS_D-Resid-ilum-Lab",
                      "HA17_SS_D-Resid-ilum-Lab",
                      "HA17_SS_D-Resid-ilum-Lab",
                      "HA17_SS_D-Resid-ilum-Lab",
                      "HA17_SS_D-Resid-ilum-Lab",
                      "HA17_SS_D-Resid-ilum-Sab",
                      "HA17_SS_D-Resid-ilum-Fest")
    ..
"Iluminacion-Residencia" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Internas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA17_HS0_SS_")
    ..
"HA18_SS_D-Resid-Func-Lab" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 0
    VALUES  = ( 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1)
    ..
"HA18_SS_D-Resid-Func-Sab" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 1
    VALUES  = ( 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1)
    ..
"HA18_SS_D-Resid-Func-Fest" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 2
    VALUES  = ( 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1, 1)
    ..
  "HA18_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = ON/OFF
    DAY-SCHEDULES = ( "HA18_SS_D-Resid-Func-Lab",
                      "HA18_SS_D-Resid-Func-Lab",
                      "HA18_SS_D-Resid-Func-Lab",
                      "HA18_SS_D-Resid-Func-Lab",
                      "HA18_SS_D-Resid-Func-Lab",
                      "HA18_SS_D-Resid-Func-Sab",
                      "HA18_SS_D-Resid-Func-Fest")
    ..
"Funcionam-Residencia" = SCHEDULE-PD
    TYPE   = "ON/OFF"
    GROUP  = "Equipos"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA18_HS0_SS_")
    ..
"HA19_SS_D-Resid-Inf-Inv" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 0
    VALUES  = ( 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25)
    ..
"HA19_SS_D-Resid-Inf-Ver" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 1
    VALUES  = ( 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25, 0.25)
    ..
  "HA19_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA19_SS_D-Resid-Inf-Inv",
                      "HA19_SS_D-Resid-Inf-Inv",
                      "HA19_SS_D-Resid-Inf-Inv",
                      "HA19_SS_D-Resid-Inf-Inv",
                      "HA19_SS_D-Resid-Inf-Inv",
                      "HA19_SS_D-Resid-Inf-Inv",
                      "HA19_SS_D-Resid-Inf-Inv")
    ..
  "HA19_HS1_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA19_SS_D-Resid-Inf-Inv",
                      "HA19_SS_D-Resid-Inf-Inv",
                      "HA19_SS_D-Resid-Inf-Inv",
                      "HA19_SS_D-Resid-Inf-Inv",
                      "HA19_SS_D-Resid-Inf-Ver",
                      "HA19_SS_D-Resid-Inf-Ver",
                      "HA19_SS_D-Resid-Inf-Ver")
    ..
  "HA19_HS2_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA19_SS_D-Resid-Inf-Ver",
                      "HA19_SS_D-Resid-Inf-Ver",
                      "HA19_SS_D-Resid-Inf-Ver",
                      "HA19_SS_D-Resid-Inf-Ver",
                      "HA19_SS_D-Resid-Inf-Ver",
                      "HA19_SS_D-Resid-Inf-Ver",
                      "HA19_SS_D-Resid-Inf-Ver")
    ..
"Infiltracion-Residencia" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Ventilación"
    MONTH = ( 5, 6, 9, 12)
    DAY   = ( 27, 3, 30, 31)
    WEEK-SCHEDULES = ( "HA19_HS0_SS_",
                       "HA19_HS1_SS_",
                       "HA19_HS2_SS_",
                       "HA19_HS0_SS_")
    ..
"HA20_SS_D-No-Habitable" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Internas"
    INDEX = 0
    VALUES  = ( 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00, 0.00)
    ..
  "HA20_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA20_SS_D-No-Habitable",
                      "HA20_SS_D-No-Habitable",
                      "HA20_SS_D-No-Habitable",
                      "HA20_SS_D-No-Habitable",
                      "HA20_SS_D-No-Habitable",
                      "HA20_SS_D-No-Habitable",
                      "HA20_SS_D-No-Habitable")
    ..
"Anual-No-Habitable" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Internas"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA20_HS0_SS_")
    ..
"HA21_SS_D-No-habitable-Func" = DAY-SCHEDULE-PD
    TYPE  = "ON/OFF"
    GROUP = "Equipos"
    INDEX = 0
    VALUES  = ( 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0)
    ..
  "HA21_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = ON/OFF
    DAY-SCHEDULES = ( "HA21_SS_D-No-habitable-Func",
                      "HA21_SS_D-No-habitable-Func",
                      "HA21_SS_D-No-habitable-Func",
                      "HA21_SS_D-No-habitable-Func",
                      "HA21_SS_D-No-habitable-Func",
                      "HA21_SS_D-No-habitable-Func",
                      "HA21_SS_D-No-habitable-Func")
    ..
"Anual-No-habitable-Func" = SCHEDULE-PD
    TYPE   = "ON/OFF"
    GROUP  = "Equipos"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA21_HS0_SS_")
    ..
"HA22_SS_D-No-habitable-Inf" = DAY-SCHEDULE-PD
    TYPE  = "FRACTION"
    GROUP = "Ventilación"
    INDEX = 0
    VALUES  = ( 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00, 1.00)
    ..
  "HA22_HS0_SS_" = WEEK-SCHEDULE-PD
    TYPE  = FRACTION
    DAY-SCHEDULES = ( "HA22_SS_D-No-habitable-Inf",
                      "HA22_SS_D-No-habitable-Inf",
                      "HA22_SS_D-No-habitable-Inf",
                      "HA22_SS_D-No-habitable-Inf",
                      "HA22_SS_D-No-habitable-Inf",
                      "HA22_SS_D-No-habitable-Inf",
                      "HA22_SS_D-No-habitable-Inf")
    ..
"Anual-No-habitable-Inf" = SCHEDULE-PD
    TYPE   = "FRACTION"
    GROUP  = "Ventilación"
    MONTH = ( 12)
    DAY   = ( 31)
    WEEK-SCHEDULES = ( "HA22_HS0_SS_")
    ..
$
$ +----------------------------+
$ | DESCRIPCIÓN DE CONDICIONES |
$ +----------------------------+
$
$
$ +------------------+
$ | PUENTES TERMICOS |
$ +------------------+
$
"FRENTE_FORJADO" = THERMAL-BRIDGE
      BRIDGE-NAME = "FRENTE_FORJADO"
      TTL         = 0.700000
      LENGTH      = 61.798836
      FRSI        = 0.450000
      ANGLE-MIN   = 135
      ANGLE-MAX   = 225
      TYPE        = SLAB
      PARTITION   = YES
    ..
"UNION_CUBIERTA" = THERMAL-BRIDGE
      BRIDGE-NAME = "UNION_CUBIERTA"
      TTL         = 0.960000
      LENGTH      = 881.239685
      FRSI        = 0.280000
      ANGLE-MIN   = 0
      ANGLE-MAX   = 135
      TYPE        = SLAB
      PARTITION   = BOTH
    ..
"ESQUINA_CONVEXA_FORJADO" = THERMAL-BRIDGE
      BRIDGE-NAME = "ESQUINA_CONVEXA_FORJADO"
      TTL         = 0.680000
      LENGTH      = 11.131013
      FRSI        = 0.030000
      ANGLE-MIN   = 225
      ANGLE-MAX   = 360
      TYPE        = SLAB
      PARTITION   = BOTH
    ..
"ESQUINA_CONCAVA_CERRAMIENTO" = THERMAL-BRIDGE
      BRIDGE-NAME = "ESQUINA_CONCAVA_CERRAMIENTO"
      TTL         = -0.160000
      LENGTH      = 20.900028
      FRSI        = 0.020000
      ANGLE-MIN   = 0
      ANGLE-MAX   = 135
      TYPE        = MASONRY
      PARTITION   = BOTH
    ..
"ESQUINA_CONVEXA_CERRAMIENTO" = THERMAL-BRIDGE
      BRIDGE-NAME = "ESQUINA_CONVEXA_CERRAMIENTO"
      TTL         = 0.110000
      LENGTH      = 40.700008
      FRSI        = 0.320000
      ANGLE-MIN   = 225
      ANGLE-MAX   = 360
      TYPE        = MASONRY
      PARTITION   = BOTH
    ..
"PILAR" = THERMAL-BRIDGE
      BRIDGE-NAME = "PILAR"
      TTL         = 1.200000
      LENGTH      = 1.000000
      FRSI        = 0.200000
      TYPE        = PILLAR
    ..
"UNION_SOLERA_PAREDEXT" = THERMAL-BRIDGE
      BRIDGE-NAME = "UNION_SOLERA_PAREDEXT"
      TTL         = 0.490000
      LENGTH      = 206.910965
      FRSI        = 0.090000
      ANGLE-MIN   = 135
      ANGLE-MAX   = 225
      TYPE        = UNDER-EXT
      PARTITION   = BOTH
    ..
"HUECO_VENTANA" = THERMAL-BRIDGE
      BRIDGE-NAME = "HUECO_VENTANA"
      TTL         = 0.596566
      LENGTH      = 815.040039
      FRSI        = 0.170000
      TYPE        = WINDOW-FRAME
    ..
$
$ +-----------------------------------------------------------------+
$ |                        Final del fichero                        |
$ +-----------------------------------------------------------------+
